From 39c7486c66bd76d182c0ad02d440d7207bccb89e Mon Sep 17 00:00:00 2001
From: Sascha Hauer <s.hauer@pengutronix.de>
Date: Fri, 2 Dec 2022 09:12:23 +0100
Subject: [PATCH 12/13] wifi: rtw88: Add rtw8822cu chipset support

Add support for the rtw8822cu chipset based on
https://github.com/ulli-kroll/rtw88-usb.git

Signed-off-by: Sascha Hauer <s.hauer@pengutronix.de>
Signed-off-by: Kalle Valo <kvalo@kernel.org>
Link: https://lore.kernel.org/r/20221202081224.2779981-11-s.hauer@pengutronix.de
---
 drivers/net/wireless/realtek/rtw88/Kconfig    | 12 +++++
 drivers/net/wireless/realtek/rtw88/Makefile   |  3 ++
 drivers/net/wireless/realtek/rtw88/rtw8822c.c | 24 ++++++++++
 .../net/wireless/realtek/rtw88/rtw8822cu.c    | 44 +++++++++++++++++++
 4 files changed, 83 insertions(+)
 create mode 100644 drivers/net/wireless/realtek/rtw88/rtw8822cu.c

--- a/drivers/net/wireless/realtek/rtw88/Kconfig
+++ b/drivers/net/wireless/realtek/rtw88/Kconfig
@@ -75,6 +75,18 @@ config RTW88_8822CE
 
 	  802.11ac PCIe wireless network adapter
 
+config RTW88_8822CU
+	tristate "Realtek 8822CU USB wireless network adapter"
+	depends on m
+	depends on USB
+	select RTW88_CORE
+	select RTW88_USB
+	select RTW88_8822C
+	help
+	  Select this option will enable support for 8822CU chipset
+
+	  802.11ac USB wireless network adapter
+
 config RTW88_8723DE
 	tristate "Realtek 8723DE PCI wireless network adapter"
 	depends on m
--- a/drivers/net/wireless/realtek/rtw88/Makefile
+++ b/drivers/net/wireless/realtek/rtw88/Makefile
@@ -35,6 +35,9 @@ rtw88_8822c-objs		:= rtw8822c.o rtw8822c
 obj-$(CPTCFG_RTW88_8822CE)	+= rtw88_8822ce.o
 rtw88_8822ce-objs		:= rtw8822ce.o
 
+obj-$(CPTCFG_RTW88_8822CU)	+= rtw88_8822cu.o
+rtw88_8822cu-objs		:= rtw8822cu.o
+
 obj-$(CPTCFG_RTW88_8723D)	+= rtw88_8723d.o
 rtw88_8723d-objs		:= rtw8723d.o rtw8723d_table.o
 
--- a/drivers/net/wireless/realtek/rtw88/rtw8822c.c
+++ b/drivers/net/wireless/realtek/rtw88/rtw8822c.c
@@ -29,6 +29,12 @@ static void rtw8822ce_efuse_parsing(stru
 	ether_addr_copy(efuse->addr, map->e.mac_addr);
 }
 
+static void rtw8822cu_efuse_parsing(struct rtw_efuse *efuse,
+				    struct rtw8822c_efuse *map)
+{
+	ether_addr_copy(efuse->addr, map->u.mac_addr);
+}
+
 static int rtw8822c_read_efuse(struct rtw_dev *rtwdev, u8 *log_map)
 {
 	struct rtw_efuse *efuse = &rtwdev->efuse;
@@ -58,6 +64,9 @@ static int rtw8822c_read_efuse(struct rt
 	case RTW_HCI_TYPE_PCIE:
 		rtw8822ce_efuse_parsing(efuse, map);
 		break;
+	case RTW_HCI_TYPE_USB:
+		rtw8822cu_efuse_parsing(efuse, map);
+		break;
 	default:
 		/* unsupported now */
 		return -ENOTSUPP;
@@ -4557,6 +4566,18 @@ static void rtw8822c_adaptivity(struct r
 	rtw_phy_set_edcca_th(rtwdev, l2h, h2l);
 }
 
+static void rtw8822c_fill_txdesc_checksum(struct rtw_dev *rtwdev,
+					  struct rtw_tx_pkt_info *pkt_info,
+					  u8 *txdesc)
+{
+	const struct rtw_chip_info *chip = rtwdev->chip;
+	size_t words;
+
+	words = (pkt_info->pkt_offset * 8 + chip->tx_pkt_desc_sz) / 2;
+
+	fill_txdesc_checksum_common(txdesc, words);
+}
+
 static const struct rtw_pwr_seq_cmd trans_carddis_to_cardemu_8822c[] = {
 	{0x0086,
 	 RTW_PWR_CUT_ALL_MSK,
@@ -4895,6 +4916,8 @@ static const struct rtw_rfe_def rtw8822c
 	[0] = RTW_DEF_RFE(8822c, 0, 0),
 	[1] = RTW_DEF_RFE(8822c, 0, 0),
 	[2] = RTW_DEF_RFE(8822c, 0, 0),
+	[3] = RTW_DEF_RFE(8822c, 0, 0),
+	[4] = RTW_DEF_RFE(8822c, 0, 0),
 	[5] = RTW_DEF_RFE(8822c, 0, 5),
 	[6] = RTW_DEF_RFE(8822c, 0, 0),
 };
@@ -4978,6 +5001,7 @@ static struct rtw_chip_ops rtw8822c_ops
 	.cfo_track		= rtw8822c_cfo_track,
 	.config_tx_path		= rtw8822c_config_tx_path,
 	.config_txrx_mode	= rtw8822c_config_trx_mode,
+	.fill_txdesc_checksum	= rtw8822c_fill_txdesc_checksum,
 
 	.coex_set_init		= rtw8822c_coex_cfg_init,
 	.coex_set_ant_switch	= NULL,
--- /dev/null
+++ b/drivers/net/wireless/realtek/rtw88/rtw8822cu.c
@@ -0,0 +1,44 @@
+// SPDX-License-Identifier: GPL-2.0 OR BSD-3-Clause
+/* Copyright(c) 2018-2019  Realtek Corporation
+ */
+
+#include <linux/module.h>
+#include <linux/usb.h>
+#include "main.h"
+#include "rtw8822c.h"
+#include "usb.h"
+
+static const struct usb_device_id rtw_8822cu_id_table[] = {
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xc82c, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822c_hw_spec) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xc812, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822c_hw_spec) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xc82e, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822c_hw_spec) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xd820, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822c_hw_spec) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(RTW_USB_VENDOR_ID_REALTEK, 0xd82b, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822c_hw_spec) },
+	{ USB_DEVICE_AND_INTERFACE_INFO(0x13b1, 0x0043, 0xff, 0xff, 0xff),
+	  .driver_info = (kernel_ulong_t)&(rtw8822c_hw_spec) }, /* Alpha - Alpha */
+	{},
+};
+MODULE_DEVICE_TABLE(usb, rtw_8822cu_id_table);
+
+static int rtw8822bu_probe(struct usb_interface *intf,
+			   const struct usb_device_id *id)
+{
+	return rtw_usb_probe(intf, id);
+}
+
+static struct usb_driver rtw_8822cu_driver = {
+	.name = "rtw_8822cu",
+	.id_table = rtw_8822cu_id_table,
+	.probe = rtw8822bu_probe,
+	.disconnect = rtw_usb_disconnect,
+};
+module_usb_driver(rtw_8822cu_driver);
+
+MODULE_AUTHOR("Realtek Corporation");
+MODULE_DESCRIPTION("Realtek 802.11ac wireless 8822cu driver");
+MODULE_LICENSE("Dual BSD/GPL");
