From a02233a1346132efe6dda33237a0b07771fbb09b Mon Sep 17 00:00:00 2001
From: Sascha Hauer <s.hauer@pengutronix.de>
Date: Fri, 2 Dec 2022 09:12:14 +0100
Subject: [PATCH 03/13] wifi: rtw88: print firmware type in info message

It's confusing to read two different firmware versions in the syslog
for the same device:

rtw_8822cu 2-1:1.2: Firmware version 9.9.4, H2C version 15
rtw_8822cu 2-1:1.2: Firmware version 9.9.11, H2C version 15

Print the firmware type in this message to make clear these are really
two different firmwares for different purposes:

rtw_8822cu 1-1.4:1.2: WOW Firmware version 9.9.4, H2C version 15
rtw_8822cu 1-1.4:1.2: Firmware version 9.9.11, H2C version 15

Signed-off-by: Sascha Hauer <s.hauer@pengutronix.de>
Reviewed-by: Ping-Ke Shih <pkshih@realtek.com>
Signed-off-by: Kalle Valo <kvalo@kernel.org>
Link: https://lore.kernel.org/r/20221202081224.2779981-2-s.hauer@pengutronix.de
---
 drivers/net/wireless/realtek/rtw88/main.c | 4 +++-
 drivers/net/wireless/realtek/rtw88/main.h | 1 +
 2 files changed, 4 insertions(+), 1 deletion(-)

--- a/drivers/net/wireless/realtek/rtw88/main.c
+++ b/drivers/net/wireless/realtek/rtw88/main.c
@@ -1746,7 +1746,8 @@ static void rtw_load_firmware_cb(const s
 	update_firmware_info(rtwdev, fw);
 	complete_all(&fw->completion);
 
-	rtw_info(rtwdev, "Firmware version %u.%u.%u, H2C version %u\n",
+	rtw_info(rtwdev, "%sFirmware version %u.%u.%u, H2C version %u\n",
+		 fw->type == RTW_WOWLAN_FW ? "WOW " : "",
 		 fw->version, fw->sub_version, fw->sub_index, fw->h2c_version);
 }
 
@@ -1772,6 +1773,7 @@ static int rtw_load_firmware(struct rtw_
 		return -ENOENT;
 	}
 
+	fw->type = type;
 	fw->rtwdev = rtwdev;
 	init_completion(&fw->completion);
 
--- a/drivers/net/wireless/realtek/rtw88/main.h
+++ b/drivers/net/wireless/realtek/rtw88/main.h
@@ -1854,6 +1854,7 @@ struct rtw_fw_state {
 	u16 h2c_version;
 	u32 feature;
 	u32 feature_ext;
+	enum rtw_fw_type type;
 };
 
 enum rtw_sar_sources {
