From 2e9bffc4f713db465177238f6033f7d367d6f151 Mon Sep 17 00:00:00 2001
From: Shawn Lin <shawn.lin@rock-chips.com>
Date: Thu, 25 Aug 2022 21:38:34 +0200
Subject: [PATCH] phy: rockchip: Support PCIe v3

RK3568 supports PCIe v3 using not Combphy like PCIe v2 on rk3566.
It use a dedicated PCIe-phy. Add support for this.

Initial support by Shawn Lin, modifications by Peter Geis and Frank
Wunderlich.

Add data-lanes property for splitting pcie-lanes across controllers.

The data-lanes is an array where x=0 means lane is disabled and  x > 0
means controller x is assigned to phy lane.

Signed-off-by: Shawn Lin <shawn.lin@rock-chips.com>
Suggested-by: Peter Geis <pgwipeout@gmail.com>
Signed-off-by: Frank Wunderlich <frank-w@public-files.de>
Link: https://lore.kernel.org/r/20220825193836.54262-4-linux@fw-web.de
Signed-off-by: Vinod Koul <vkoul@kernel.org>
---
 drivers/phy/rockchip/Kconfig                  |   9 +
 drivers/phy/rockchip/Makefile                 |   1 +
 .../phy/rockchip/phy-rockchip-snps-pcie3.c    | 319 ++++++++++++++++++
 include/linux/phy/pcie.h                      |  12 +
 4 files changed, 341 insertions(+)
 create mode 100644 drivers/phy/rockchip/phy-rockchip-snps-pcie3.c
 create mode 100644 include/linux/phy/pcie.h

--- a/drivers/phy/rockchip/Kconfig
+++ b/drivers/phy/rockchip/Kconfig
@@ -83,6 +83,15 @@ config PHY_ROCKCHIP_PCIE
 	help
 	  Enable this to support the Rockchip PCIe PHY.
 
+config PHY_ROCKCHIP_SNPS_PCIE3
+	tristate "Rockchip Snps PCIe3 PHY Driver"
+	depends on (ARCH_ROCKCHIP && OF) || COMPILE_TEST
+	depends on HAS_IOMEM
+	select GENERIC_PHY
+	select MFD_SYSCON
+	help
+	  Enable this to support the Rockchip snps PCIe3 PHY.
+
 config PHY_ROCKCHIP_TYPEC
 	tristate "Rockchip TYPEC PHY Driver"
 	depends on OF && (ARCH_ROCKCHIP || COMPILE_TEST)
--- a/drivers/phy/rockchip/Makefile
+++ b/drivers/phy/rockchip/Makefile
@@ -8,5 +8,6 @@ obj-$(CONFIG_PHY_ROCKCHIP_INNO_HDMI)	+=
 obj-$(CONFIG_PHY_ROCKCHIP_INNO_USB2)	+= phy-rockchip-inno-usb2.o
 obj-$(CONFIG_PHY_ROCKCHIP_NANENG_COMBO_PHY)	+= phy-rockchip-naneng-combphy.o
 obj-$(CONFIG_PHY_ROCKCHIP_PCIE)		+= phy-rockchip-pcie.o
+obj-$(CONFIG_PHY_ROCKCHIP_SNPS_PCIE3)	+= phy-rockchip-snps-pcie3.o
 obj-$(CONFIG_PHY_ROCKCHIP_TYPEC)	+= phy-rockchip-typec.o
 obj-$(CONFIG_PHY_ROCKCHIP_USB)		+= phy-rockchip-usb.o
