From a319687ac18dcc557a88054282508e061ad8495f Mon Sep 17 00:00:00 2001
From: John Crispin <john@phrozen.org>
Date: Thu, 10 Aug 2017 14:42:19 +0200
Subject: [PATCH 31/57] net: dsa: dsa api compat

make the latest driver work on the old API

Signed-off-by: John Crispin <john@phrozen.org>
---
 drivers/net/dsa/mt7530.c | 14 ++++++++------
 drivers/net/dsa/mt7530.h |  2 ++
 net/dsa/tag_mtk.c        |  2 +-
 3 files changed, 11 insertions(+), 7 deletions(-)

--- a/drivers/net/dsa/mt7530.c
+++ b/drivers/net/dsa/mt7530.c
@@ -834,6 +834,7 @@ mt7530_port_bridge_join(struct dsa_switc
 	int i;
 
 	mutex_lock(&priv->reg_mutex);
+	priv->bridge_dev[port] = bridge;
 
 	for (i = 0; i < MT7530_NUM_PORTS; i++) {
 		/* Add this port to the port matrix of the other ports in the
@@ -841,7 +842,7 @@ mt7530_port_bridge_join(struct dsa_switc
 		 * and not being setup until the port becomes enabled.
 		 */
 		if (ds->enabled_port_mask & BIT(i) && i != port) {
-			if (ds->ports[i].bridge_dev != bridge)
+			if (priv->bridge_dev[i] != bridge)
 				continue;
 			if (priv->ports[i].enable)
 				mt7530_set(priv, MT7530_PCR_P(i),
@@ -864,8 +865,7 @@ mt7530_port_bridge_join(struct dsa_switc
 }
 
 static void
-mt7530_port_bridge_leave(struct dsa_switch *ds, int port,
-			 struct net_device *bridge)
+mt7530_port_bridge_leave(struct dsa_switch *ds, int port)
 {
 	struct mt7530_priv *priv = ds->priv;
 	int i;
@@ -878,7 +878,7 @@ mt7530_port_bridge_leave(struct dsa_swit
 		 * is kept and not being setup until the port becomes enabled.
 		 */
 		if (ds->enabled_port_mask & BIT(i) && i != port) {
-			if (ds->ports[i].bridge_dev != bridge)
+			if (priv->bridge_dev[i] != priv->bridge_dev[port])
 				continue;
 			if (priv->ports[i].enable)
 				mt7530_clear(priv, MT7530_PCR_P(i),
@@ -890,6 +890,7 @@ mt7530_port_bridge_leave(struct dsa_swit
 	/* Set the cpu port to be the only one in the port matrix of
 	 * this port.
 	 */
+	priv->bridge_dev[port] = NULL;
 	if (priv->ports[port].enable)
 		mt7530_rmw(priv, MT7530_PCR_P(port), PCR_MATRIX_MASK,
 			   PCR_MATRIX(BIT(MT7530_CPU_PORT)));
@@ -1033,7 +1034,7 @@ mt7530_probe(struct mdio_device *mdiodev
 	if (!priv)
 		return -ENOMEM;
 
-	priv->ds = dsa_switch_alloc(&mdiodev->dev, DSA_MAX_PORTS);
+	priv->ds = devm_kzalloc(&mdiodev->dev, sizeof(*priv->ds), GFP_KERNEL);
 	if (!priv->ds)
 		return -ENOMEM;
 
@@ -1076,12 +1077,13 @@ mt7530_probe(struct mdio_device *mdiodev
 	priv->bus = mdiodev->bus;
 	priv->dev = &mdiodev->dev;
 	priv->ds->priv = priv;
+	priv->ds->dev = &mdiodev->dev;
 	priv->ds->ops = &mt7530_switch_ops;
 	mutex_init(&priv->reg_mutex);
 	lpriv = priv;
 	dev_set_drvdata(&mdiodev->dev, priv);
 
-	return dsa_register_switch(priv->ds, &mdiodev->dev);
+	return dsa_register_switch(priv->ds, priv->ds->dev->of_node);
 }
 
 static void
--- a/drivers/net/dsa/mt7530.h
+++ b/drivers/net/dsa/mt7530.h
@@ -379,6 +379,8 @@ struct mt7530_priv {
 	struct mt7530_port	ports[MT7530_NUM_PORTS];
 	/* protect among processes for registers access*/
 	struct mutex reg_mutex;
+
+	struct net_device *bridge_dev[MT7530_NUM_PORTS];
 };
 
 struct mt7530_hw_stats {
--- a/net/dsa/tag_mtk.c
+++ b/net/dsa/tag_mtk.c
@@ -35,7 +35,7 @@ static struct sk_buff *mtk_tag_xmit(stru
 	/* Build the tag after the MAC Source Address */
 	mtk_tag = skb->data + 2 * ETH_ALEN;
 	mtk_tag[0] = 0;
-	mtk_tag[1] = (1 << p->dp->index) & MTK_HDR_XMIT_DP_BIT_MASK;
+	mtk_tag[1] = (1 << p->port) & MTK_HDR_XMIT_DP_BIT_MASK;
 	mtk_tag[2] = 0;
 	mtk_tag[3] = 0;
 
