From 52e9ce30a2b3c414e0efb20632fefa7cfc5096e6 Mon Sep 17 00:00:00 2001
From: John Crispin <john@phrozen.org>
Date: Thu, 10 Aug 2017 14:44:18 +0200
Subject: [PATCH 32/57] net: dsa: mediatek: add support for GMAC2 wired to ext
 phy

Signed-off-by: John Crispin <john@phrozen.org>
---
 drivers/net/dsa/mt7530.c                    | 5 +++++
 drivers/net/ethernet/mediatek/mtk_eth_soc.c | 3 +++
 2 files changed, 8 insertions(+)

--- a/drivers/net/dsa/mt7530.c
+++ b/drivers/net/dsa/mt7530.c
@@ -629,6 +629,11 @@ mt7530_setup(struct dsa_switch *ds)
 	val = mt7530_read(priv, MT7530_MHWTRAP);
 	val &= ~MHWTRAP_P6_DIS & ~MHWTRAP_PHY_ACCESS;
 	val |= MHWTRAP_MANUAL;
+	if (!dsa_is_cpu_port(ds, 5)) {
+		val |= MHWTRAP_P5_DIS;
+		val |= MHWTRAP_P5_MAC_SEL;
+		val |= MHWTRAP_P5_RGMII_MODE;
+	}
 	mt7530_write(priv, MT7530_MHWTRAP, val);
 
 	/* Enable and reset MIB counters */
--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -221,6 +221,9 @@ static void mtk_phy_link_adjust(struct n
 		netif_carrier_on(dev);
 	else
 		netif_carrier_off(dev);
+
+	if (!of_phy_is_fixed_link(mac->of_node))
+		phy_print_status(dev->phydev);
 }
 
 static int mtk_phy_connect_node(struct mtk_eth *eth, struct mtk_mac *mac,
