From eeacbb3e30f220d5d775c61421f813d4e186a325 Mon Sep 17 00:00:00 2001
From: Dan Haab <dhaab@luxul.com>
Date: Sat, 14 Jan 2017 19:29:27 -0700
Subject: [PATCH] ARM: BCM5301X: Add DT for Luxul XAP-1410

Luxul XAP-1410 in a dual-band access point device based on BCM47081 with
serial flash. It has 3 LEDs and just one (reset) button.

Signed-off-by: Dan Haab <dhaab@luxul.com>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/Makefile                    |  1 +
 arch/arm/boot/dts/bcm47081-luxul-xap-1410.dts | 60 +++++++++++++++++++++++++++
 2 files changed, 61 insertions(+)
 create mode 100644 arch/arm/boot/dts/bcm47081-luxul-xap-1410.dts

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -73,6 +73,7 @@ dtb-$(CONFIG_ARCH_BCM_5301X) += \
 	bcm47081-asus-rt-n18u.dtb \
 	bcm47081-buffalo-wzr-600dhp2.dtb \
 	bcm47081-buffalo-wzr-900dhp.dtb \
+	bcm47081-luxul-xap-1410.dtb \
 	bcm4709-asus-rt-ac87u.dtb \
 	bcm4709-buffalo-wxr-1900dhp.dtb \
 	bcm4709-netgear-r7000.dtb \
--- /dev/null
+++ b/arch/arm/boot/dts/bcm47081-luxul-xap-1410.dts
@@ -0,0 +1,60 @@
+/*
+ * Copyright 2017 Luxul Inc.
+ *
+ * Licensed under the ISC license.
+ */
+
+/dts-v1/;
+
+#include "bcm47081.dtsi"
+
+/ {
+	compatible = "luxul,xap-1410v1", "brcm,bcm47081", "brcm,bcm4708";
+	model = "Luxul XAP-1410 V1";
+
+	chosen {
+		bootargs = "console=ttyS0,115200";
+	};
+
+	memory {
+		reg = <0x00000000 0x08000000>;
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		5ghz {
+			label = "bcm53xx:blue:5ghz";
+			gpios = <&chipcommon 13 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "none";
+		};
+
+		2ghz {
+			label = "bcm53xx:blue:2ghz";
+			gpios = <&chipcommon 14 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "none";
+		};
+
+		status {
+			label = "bcm53xx:green:status";
+			gpios = <&chipcommon 15 GPIO_ACTIVE_LOW>;
+			linux,default-trigger = "timer";
+		};
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		restart {
+			label = "Reset";
+			linux,code = <KEY_RESTART>;
+			gpios = <&chipcommon 11 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
+
+&spi_nor {
+	status = "okay";
+};
