From 3dc9eca8ece2934047f1d5c290fd36c0e8698756 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Thu, 23 Feb 2017 14:06:36 +0100
Subject: [PATCH] ARM: dts: BCM5301X: Add basic DT for Linksys EA9500
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

It's tri-band wireless home router based on BCM47094 AKA BCM4709C0. It
uses 3 x BCM4366 chipsets for wireless.
Panamera seems to be board name used by Linksys.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm/boot/dts/Makefile                      |  1 +
 arch/arm/boot/dts/bcm47094-linksys-panamera.dts | 36 +++++++++++++++++++++++++
 2 files changed, 37 insertions(+)
 create mode 100644 arch/arm/boot/dts/bcm47094-linksys-panamera.dts

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -93,6 +93,7 @@ dtb-$(CONFIG_ARCH_BCM_5301X) += \
 	bcm4709-netgear-r8000.dtb \
 	bcm4709-tplink-archer-c9-v1.dtb \
 	bcm47094-dlink-dir-885l.dtb \
+	bcm47094-linksys-panamera.dtb \
 	bcm47094-luxul-xwr-3100.dtb \
 	bcm47094-netgear-r8500.dtb \
 	bcm94708.dtb \
--- /dev/null
+++ b/arch/arm/boot/dts/bcm47094-linksys-panamera.dts
@@ -0,0 +1,36 @@
+/*
+ * Copyright (C) 2017 Rafał Miłecki <rafal@milecki.pl>
+ *
+ * Licensed under the ISC license.
+ */
+
+/dts-v1/;
+
+#include "bcm47094.dtsi"
+#include "bcm5301x-nand-cs0-bch8.dtsi"
+
+/ {
+	compatible = "linksys,panamera", "brcm,bcm47094", "brcm,bcm4708";
+	model = "Linksys EA9500";
+
+	chosen {
+		bootargs = "console=ttyS0,115200";
+	};
+
+	memory {
+		reg = <0x00000000 0x08000000
+		       0x88000000 0x08000000>;
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		wps {
+			label = "WPS";
+			linux,code = <KEY_WPS_BUTTON>;
+			gpios = <&chipcommon 3 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
