From 6375219951a66047805ed977b674615d152001ee Mon Sep 17 00:00:00 2001
From: Brian Norris <computersforpeace@gmail.com>
Date: Fri, 30 Oct 2015 20:33:23 -0700
Subject: [PATCH 04/11] mtd: nand: convert to nand_set_flash_node()

Used semantic patch with 'make coccicheck MODE=patch COCCI=script.cocci':

---8<----
virtual patch

@@
struct nand_chip *c;
struct device_node *d;
@@
-(c)->flash_node = (d)
+nand_set_flash_node(c, d)
---8<----

Signed-off-by: Brian Norris <computersforpeace@gmail.com>
Reviewed-by: Marek Vasut <marex@denx.de>
Reviewed-by: Boris Brezillon <boris.brezillon@free-electrons.com>
---
 drivers/mtd/nand/brcmnand/brcmnand.c | 2 +-
 drivers/mtd/nand/fsmc_nand.c         | 2 +-
 drivers/mtd/nand/sunxi_nand.c        | 2 +-
 drivers/mtd/nand/vf610_nfc.c         | 2 +-
 4 files changed, 4 insertions(+), 4 deletions(-)

--- a/drivers/mtd/nand/brcmnand/brcmnand.c
+++ b/drivers/mtd/nand/brcmnand/brcmnand.c
@@ -1957,7 +1957,7 @@ static int brcmnand_init_cs(struct brcmn
 	mtd = &host->mtd;
 	chip = &host->chip;
 
-	chip->flash_node = dn;
+	nand_set_flash_node(chip, dn);
 	chip->priv = host;
 	mtd->priv = chip;
 	mtd->name = devm_kasprintf(&pdev->dev, GFP_KERNEL, "brcmnand.%d",
--- a/drivers/mtd/nand/fsmc_nand.c
+++ b/drivers/mtd/nand/fsmc_nand.c
@@ -1033,7 +1033,7 @@ static int __init fsmc_nand_probe(struct
 	nand->options = pdata->options;
 	nand->select_chip = fsmc_select_chip;
 	nand->badblockbits = 7;
-	nand->flash_node = np;
+	nand_set_flash_node(nand, np);
 
 	if (pdata->width == FSMC_NAND_BW16)
 		nand->options |= NAND_BUSWIDTH_16;
--- a/drivers/mtd/nand/sunxi_nand.c
+++ b/drivers/mtd/nand/sunxi_nand.c
@@ -1330,7 +1330,7 @@ static int sunxi_nand_chip_init(struct d
 	 * in the DT.
 	 */
 	nand->ecc.mode = NAND_ECC_HW;
-	nand->flash_node = np;
+	nand_set_flash_node(nand, np);
 	nand->select_chip = sunxi_nfc_select_chip;
 	nand->cmd_ctrl = sunxi_nfc_cmd_ctrl;
 	nand->read_buf = sunxi_nfc_read_buf;
--- a/drivers/mtd/nand/vf610_nfc.c
+++ b/drivers/mtd/nand/vf610_nfc.c
@@ -714,7 +714,7 @@ static int vf610_nfc_probe(struct platfo
 				goto error;
 			}
 
-			chip->flash_node = child;
+			nand_set_flash_node(chip, child);
 		}
 	}
 
