/dts-v1/;

#include "rt2880.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	#address-cells = <1>;
	#size-cells = <1>;
	compatible = "buffalo,wzr-agl300nh", "ralink,rt2880-soc";
	model = "Buffalo WZR-AGL300NH";

	pci@440000 {
		status = "ok";
	};

	cfi@1f000000 {
		compatible = "cfi-flash";
		reg = <0x1f000000 0x800000>;
		bank-width = <2>;
		device-width = <2>;
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "uboot";
			reg = <0x0 0x30000>;
			read-only;
		};

		partition@30000 {
			label = "uboot-env";
			reg = <0x30000 0x10000>;
			read-only;
		};

		factory: partition@40000 {
			label = "factory";
			reg = <0x40000 0x10000>;
			read-only;
		};

		partition@50000 {
			label = "firmware";
			reg = <0x50000 0x3b0000>;
		};
	};

	rtl8366s {
		compatible = "realtek,rtl8366s";
		gpio-sda = <&gpio0 1 GPIO_ACTIVE_HIGH>;
		gpio-sck = <&gpio0 2 GPIO_ACTIVE_HIGH>;
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <100>;

		wps {
			label = "wps";
			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		router {
			label = "router_switch";
			gpios = <&gpio0 7 GPIO_ACTIVE_HIGH>;
			linux,code = <BTN_0>;
		};

		reset {
			label = "reset";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		router {
			label = "wzr-agl300nh:green:router";
			gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
		};

		diag {
			label = "wzr-agl300nh:red:diag";
			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
		};

		security_g {
			label = "wzr-agl300nh:orange:security_g";
			gpios = <&gpio0 11 GPIO_ACTIVE_LOW>;
		};

		security_n {
			label = "wzr-agl300nh:orange:security_n";
			gpios = <&gpio0 13 GPIO_ACTIVE_LOW>;
		};
	};
};

&gpio0 {
	status = "okay";
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "i2c", "uartlite", "mdio";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	status = "okay";
	mtd-mac-address = <&factory 0x4>;

	port@0 {
		mediatek,fixed-link = <1000 1 1 1>;
	};

	mdio-bus {
		status = "okay";

		phy0: ethernet-phy@0 {
			phy-mode = "mii";
			reg = <0>;
		};
	};
};

&wmac {
	ralink,mtd-eeprom = <&factory 0>;
};
