From 39d2882058345b5994680b8731848a0343878019 Mon Sep 17 00:00:00 2001
From: Jonas Gorski <jonas.gorski@gmail.com>
Date: Sat, 4 Feb 2017 12:58:50 +0100
Subject: [PATCH 7/8] MIPS: BCM63XX: do not register SPI controllers

We now register them through DT, so no need to keep them here.

Signed-off-by: Jonas Gorski <jonas.gorski@gmail.com>
---
 arch/mips/bcm63xx/boards/board_bcm963xx.c | 7 -------
 1 file changed, 7 deletions(-)

--- a/arch/mips/bcm63xx/boards/board_common.c
+++ b/arch/mips/bcm63xx/boards/board_common.c
@@ -28,9 +28,7 @@
 #include <bcm63xx_dev_enet.h>
 #include <bcm63xx_dev_dsp.h>
 #include <bcm63xx_dev_flash.h>
-#include <bcm63xx_dev_hsspi.h>
 #include <bcm63xx_dev_pcmcia.h>
-#include <bcm63xx_dev_spi.h>
 #include <bcm63xx_dev_usb_ehci.h>
 #include <bcm63xx_dev_usb_ohci.h>
 #include <bcm63xx_dev_usb_usbd.h>
@@ -240,10 +238,6 @@ int __init board_register_devices(void)
 	     bcm63xx_register_fallback_sprom(&board.fallback_sprom)))
 		pr_err(PFX "failed to register fallback SPROM\n");
 
-	bcm63xx_spi_register();
-
-	bcm63xx_hsspi_register();
-
 	bcm63xx_flash_register();
 
 	bcm63xx_led_data.num_leds = ARRAY_SIZE(board.leds);
