The fref and the tcxo clocks settings are optional in some platforms.
WiLink8 doesn't need either, so we don't check the values.  WiLink 6
only needs the fref clock, so we check that it is valid or return with
an error.  WiLink7 needs both clocks, if either is not available we
return with an error.

Signed-off-by: Luciano Coelho <coelho@ti.com>
Reviewed-by: Felipe Balbi <balbi@ti.com>

--- a/drivers/net/wireless/ti/wl12xx/main.c
+++ b/drivers/net/wireless/ti/wl12xx/main.c
@@ -930,6 +930,11 @@ static int wl128x_boot_clk(struct wl1271
 	u16 sys_clk_cfg;
 	int ret;
 
+	if ((priv->ref_clock < 0) || (priv->tcxo_clock < 0)) {
+		wl1271_error("Missing fref and/or tcxo clock settings\n");
+		return -EINVAL;
+	}
+
 	/* For XTAL-only modes, FREF will be used after switching from TCXO */
 	if (priv->ref_clock == WL12XX_REFCLOCK_26_XTAL ||
 	    priv->ref_clock == WL12XX_REFCLOCK_38_XTAL) {
@@ -979,6 +984,11 @@ static int wl127x_boot_clk(struct wl1271
 	u32 clk;
 	int ret;
 
+	if (priv->ref_clock < 0) {
+		wl1271_error("Missing fref clock settings\n");
+		return -EINVAL;
+	}
+
 	if (WL127X_PG_GET_MAJOR(wl->hw_pg_ver) < 3)
 		wl->quirks |= WLCORE_QUIRK_END_OF_TRANSACTION;
 
@@ -1768,7 +1778,7 @@ static int wl12xx_setup(struct wl1271 *w
 	wlcore_set_ht_cap(wl, IEEE80211_BAND_5GHZ, &wl12xx_ht_cap);
 	wl12xx_conf_init(wl);
 
-	if (!fref_param) {
+	if (!fref_param && (pdata->ref_clock_freq > 0)) {
 		priv->ref_clock = wl12xx_get_clock_idx(wl12xx_refclock_table,
 						       pdata->ref_clock_freq,
 						       pdata->ref_clock_xtal);
@@ -1779,6 +1789,8 @@ static int wl12xx_setup(struct wl1271 *w
 
 			return priv->ref_clock;
 		}
+	} else if (!fref_param) {
+		priv->ref_clock = -EINVAL;
 	} else {
 		if (!strcmp(fref_param, "19.2"))
 			priv->ref_clock = WL12XX_REFCLOCK_19;
@@ -1796,7 +1808,7 @@ static int wl12xx_setup(struct wl1271 *w
 			wl1271_error("Invalid fref parameter %s", fref_param);
 	}
 
-	if (!tcxo_param) {
+	if (!fref_param && (pdata->tcxo_clock_freq > 0)) {
 		priv->tcxo_clock = wl12xx_get_clock_idx(wl12xx_tcxoclock_table,
 							pdata->tcxo_clock_freq,
 							true);
@@ -1806,7 +1818,9 @@ static int wl12xx_setup(struct wl1271 *w
 
 			return priv->tcxo_clock;
 		}
-	} else {
+	} else if (!fref_param) {
+		priv->tcxo_clock = -EINVAL;
+	}else {
 		if (!strcmp(tcxo_param, "19.2"))
 			priv->tcxo_clock = WL12XX_TCXOCLOCK_19_2;
 		else if (!strcmp(tcxo_param, "26"))
--- a/drivers/net/wireless/ti/wlcore/sdio.c
+++ b/drivers/net/wireless/ti/wlcore/sdio.c
@@ -252,20 +252,16 @@ static struct wl12xx_platform_data *wlco
 	for_each_matching_node(clock_node, wlcore_sdio_of_clk_match_table)
 		of_fixed_clk_setup(clock_node);
 
-	/* TODO: make sure we have this when needed (ie. for WL6 and WL7) */
 	glue->refclock = of_clk_get_by_name(np, "refclock");
 	if (IS_ERR(glue->refclock)) {
-		dev_err(dev, "couldn't find refclock on the device tree\n");
 		glue->refclock = NULL;
 	} else {
 		clk_prepare_enable(glue->refclock);
 		pdata->ref_clock_freq = clk_get_rate(glue->refclock);
 	}
 
-	/* TODO: make sure we have this when needed (ie. for WL7) */
 	glue->tcxoclock = of_clk_get_by_name(np, "tcxoclock");
 	if (IS_ERR(glue->tcxoclock)) {
-		dev_err(dev, "couldn't find tcxoclock on the device tree\n");
 		glue->tcxoclock = NULL;
 	} else {
 		clk_prepare_enable(glue->tcxoclock);
