Register switch connected to srab

Signed-off-by: Hauke Mehrtens <hauke@hauke-m.de>

--- a/drivers/net/ethernet/broadcom/bgmac.c
+++ b/drivers/net/ethernet/broadcom/bgmac.c
@@ -16,6 +16,7 @@
 #include <linux/phy.h>
 #include <linux/interrupt.h>
 #include <linux/dma-mapping.h>
+#include <linux/platform_data/b53.h>
 #include <bcm47xx_nvram.h>
 
 static const struct bcma_device_id bgmac_bcma_tbl[] = {
@@ -1443,6 +1444,17 @@ static void bgmac_mii_unregister(struct
 	mdiobus_free(mii_bus);
 }
 
+static struct b53_platform_data bgmac_b53_pdata = {
+};
+
+static struct platform_device bgmac_b53_dev = {
+	.name		= "b53-srab-switch",
+	.id		= -1,
+	.dev		= {
+		.platform_data = &bgmac_b53_pdata,
+	},
+};
+
 /**************************************************
  * BCMA bus ops
  **************************************************/
@@ -1561,6 +1573,16 @@ static int bgmac_probe(struct bcma_devic
 		goto err_dma_free;
 	}
 
+	if (core->id.id != BCMA_CHIP_ID_BCM4707 &&
+	    core->id.id != BCMA_CHIP_ID_BCM53018 &&
+	    !bgmac_b53_pdata.regs) {
+		bgmac_b53_pdata.regs = ioremap_nocache(0x18007000, 0x1000);
+
+		err = platform_device_register(&bgmac_b53_dev);
+		if (!err)
+			bgmac->b53_device = &bgmac_b53_dev;
+	}
+
 	err = register_netdev(bgmac->net_dev);
 	if (err) {
 		bgmac_err(bgmac, "Cannot register net device\n");
@@ -1590,6 +1612,10 @@ static void bgmac_remove(struct bcma_dev
 {
 	struct bgmac *bgmac = bcma_get_drvdata(core);
 
+	if (bgmac->b53_device)
+		platform_device_unregister(&bgmac_b53_dev);
+	bgmac->b53_device = NULL;
+
 	netif_napi_del(&bgmac->napi);
 	unregister_netdev(bgmac->net_dev);
 	bgmac_mii_unregister(bgmac);
--- a/drivers/net/ethernet/broadcom/bgmac.h
+++ b/drivers/net/ethernet/broadcom/bgmac.h
@@ -430,6 +430,9 @@ struct bgmac {
 	bool has_robosw;
 
 	bool loopback;
+
+	/* platform device for associated switch */
+	struct platform_device *b53_device;
 };
 
 static inline u32 bgmac_read(struct bgmac *bgmac, u16 offset)
