/*
 * Copyright (C) 2013 Michael Heimpold <mhei@heimpold.de>
 *
 * The code contained herein is licensed under the GNU General Public
 * License. You may obtain a copy of the GNU General Public License
 * Version 2 or later at the following locations:
 *
 * http://www.opensource.org/licenses/gpl-license.html
 * http://www.gnu.org/copyleft/gpl.html
 */

/dts-v1/;
/include/ "imx28.dtsi"

/ {
	model = "I2SE Duckbill";
	compatible = "i2se,duckbill", "fsl,imx28";

	memory {
		reg = <0x40000000 0x08000000>;
	};

	apb@80000000 {
		apbh@80000000 {
			ssp0: ssp@80010000 {
				compatible = "fsl,imx28-mmc";
				pinctrl-names = "default";
				pinctrl-0 = <&mmc0_8bit_pins_a
					&mmc0_cd_cfg &mmc0_sck_cfg>;
				bus-width = <8>;
				vmmc-supply = <&reg_3p3v>;
				status = "okay";
			};

			pinctrl@80018000 {
				pinctrl-names = "default";
				pinctrl-0 = <&hog_pins_a>;

				hog_pins_a: hog@0 {
					reg = <0>;
					fsl,pinmux-ids = <
						0x40d3 /* MX28_PAD_ENET0_RX_CLK__GPIO_4_13, PHY Reset */
					>;
					fsl,drive-strength = <0>;
					fsl,voltage = <1>;
					fsl,pull-up = <0>;
				};

				led_pins_a: led_gpio@0 {
					reg = <0>;
					fsl,pinmux-ids = <
						0x3043 /* MX28_PAD_AUART1_RX__GPIO_3_4 */
						0x3053 /* MX28_PAD_AUART1_TX__GPIO_3_5 */
					>;
					fsl,drive-strength = <0>;
					fsl,voltage = <1>;
					fsl,pull-up = <0>;
				};
			};
		};

		apbx@80040000 {
			duart: serial@80074000 {
				pinctrl-names = "default";
				pinctrl-0 = <&duart_pins_a>;
				status = "okay";
			};

			usbphy0: usbphy@8007c000 {
				status = "okay";
			};
		};
	};

	ahb@80080000 {
		usb0: usb@80080000 {
			status = "okay";
		};

		mac0: ethernet@800f0000 {
			phy-mode = "rmii";
			pinctrl-names = "default";
			pinctrl-0 = <&mac0_pins_a>;
			phy-supply = <&reg_3p3v>;
			phy-reset-gpios = <&gpio4 13 0>;
			phy-reset-duration = <100>;
			status = "okay";
		};
	};

	regulators {
		compatible = "simple-bus";

		reg_3p3v: 3p3v {
			compatible = "regulator-fixed";
			regulator-name = "3P3V";
			regulator-min-microvolt = <3300000>;
			regulator-max-microvolt = <3300000>;
			regulator-always-on;
		};
	};

	leds {
		compatible = "gpio-leds";
		pinctrl-names = "default";
		pinctrl-0 = <&led_pins_a>;

		status {
			label = "duckbill:green:status";
			gpios = <&gpio3 5 0>;
		};

		failure {
			label = "duckbill:red:status";
			gpios = <&gpio3 4 0>;
		};
	};
};
