--- a/include/configs/wandboard.h
+++ b/include/configs/wandboard.h
@@ -48,7 +48,7 @@
 #define CONFIG_CMD_BMODE
 #define CONFIG_CMD_SETEXPR
 
-#define CONFIG_BOOTDELAY		5
+#define CONFIG_BOOTDELAY		3
 
 #define CONFIG_SYS_MEMTEST_START	0x10000000
 #define CONFIG_SYS_MEMTEST_END		(CONFIG_SYS_MEMTEST_START + 500 * SZ_1M)
@@ -101,13 +101,15 @@
 
 #if defined(CONFIG_MX6DL) || defined(CONFIG_MX6S)
 #define CONFIG_DEFAULT_FDT_FILE		"imx6dl-wandboard.dtb"
+#define CONFIG_OWRT_NAME		"openwrt-imx6-imx6dl-wandboard-fit-uImage.itb"
 #elif defined(CONFIG_MX6Q)
 #define CONFIG_DEFAULT_FDT_FILE		"imx6q-wandboard.dtb"
+#define CONFIG_OWRT_NAME		"openwrt-imx6-imx6q-wandboard-fit-uImage.itb"
 #endif
 
 #define CONFIG_EXTRA_ENV_SETTINGS \
 	"script=boot.scr\0" \
-	"uimage=uImage\0" \
+	"uimage=" CONFIG_OWRT_NAME "\0" \
 	"console=ttymxc0\0" \
 	"splashpos=m,m\0" \
 	"fdt_high=0xffffffff\0" \
@@ -136,11 +138,11 @@
 	"mmcargs=setenv bootargs console=${console},${baudrate} " \
 		"root=${mmcroot}\0" \
 	"loadbootscript=" \
-		"fatload mmc ${mmcdev}:${mmcpart} ${loadaddr} ${script};\0" \
+		"ext2load mmc ${mmcdev}:${mmcpart} ${loadaddr} ${script};\0" \
 	"bootscript=echo Running bootscript from mmc ...; " \
 		"source\0" \
-	"loaduimage=fatload mmc ${mmcdev}:${mmcpart} ${loadaddr} ${uimage}\0" \
-	"loadfdt=fatload mmc ${mmcdev}:${mmcpart} ${fdt_addr} ${fdt_file}\0" \
+	"loaduimage=ext2load mmc ${mmcdev}:${mmcpart} ${loadaddr} ${uimage}\0" \
+	"loadfdt=ext2load mmc ${mmcdev}:${mmcpart} ${fdt_addr} ${fdt_file}\0" \
 	"mmcboot=echo Booting from mmc ...; " \
 		"run mmcargs; " \
 		"if test ${boot_fdt} = yes || test ${boot_fdt} = try; then " \
@@ -155,30 +157,6 @@
 			"fi; " \
 		"else " \
 			"bootm; " \
-		"fi;\0" \
-	"netargs=setenv bootargs console=${console},${baudrate} " \
-		"root=/dev/nfs " \
-	"ip=dhcp nfsroot=${serverip}:${nfsroot},v3,tcp\0" \
-		"netboot=echo Booting from net ...; " \
-		"run netargs; " \
-		"if test ${ip_dyn} = yes; then " \
-			"setenv get_cmd dhcp; " \
-		"else " \
-			"setenv get_cmd tftp; " \
-		"fi; " \
-		"${get_cmd} ${uimage}; " \
-		"if test ${boot_fdt} = yes || test ${boot_fdt} = try; then " \
-			"if ${get_cmd} ${fdt_addr} ${fdt_file}; then " \
-				"bootm ${loadaddr} - ${fdt_addr}; " \
-			"else " \
-				"if test ${boot_fdt} = try; then " \
-					"bootm; " \
-				"else " \
-					"echo WARN: Cannot load the DT; " \
-				"fi; " \
-			"fi; " \
-		"else " \
-			"bootm; " \
 		"fi;\0"
 
 #define CONFIG_BOOTCOMMAND \
@@ -188,10 +166,10 @@
 		   "else " \
 			   "if run loaduimage; then " \
 				   "run mmcboot; " \
-			   "else run netboot; " \
+			   "else echo WARN: Can not boot the image; " \
 			   "fi; " \
 		   "fi; " \
-	   "else run netboot; fi"
+	   "fi"
 
 /* Miscellaneous configurable options */
 #define CONFIG_SYS_LONGHELP
