From aaf8700dfa1b19bbb994e2996bd293190c0cefbd Mon Sep 17 00:00:00 2001
From: arokux <arokux@gmail.com>
Date: Sun, 6 Oct 2013 14:04:50 +0200
Subject: [PATCH] clk: sun5i: Add support for USB clocks

---
 drivers/clk/sunxi/clk-sunxi.c | 5 +++++
 1 file changed, 5 insertions(+)

diff --git a/drivers/clk/sunxi/clk-sunxi.c b/drivers/clk/sunxi/clk-sunxi.c
index cbe1516..f9b8b18 100644
--- a/drivers/clk/sunxi/clk-sunxi.c
+++ b/drivers/clk/sunxi/clk-sunxi.c
@@ -623,6 +623,10 @@ struct gates_data {
 	.mask = {0x1C0},
 };
 
+static const struct gates_data sun5i_usb_gates_data __initconst = {
+       .mask = {0x140},
+};
+
 static const struct gates_data sun5i_a10s_ahb_gates_data __initconst = {
 	.mask = {0x147667e7, 0x185915},
 };
@@ -874,6 +878,7 @@ static void __init sunxi_divs_clk_setup(struct device_node *node,
 	{.compatible = "allwinner,sun47i-usb-gates-clk", .data = &sun47i_usb_gates_data,},
 	{.compatible = "allwinner,sun5i-a10s-ahb-gates-clk", .data = &sun5i_a10s_ahb_gates_data,},
 	{.compatible = "allwinner,sun5i-a13-ahb-gates-clk", .data = &sun5i_a13_ahb_gates_data,},
+	{.compatible = "allwinner,sun5i-usb-gates-clk", .data = &sun5i_usb_gates_data,},
 	{.compatible = "allwinner,sun6i-a31-ahb1-gates-clk", .data = &sun6i_a31_ahb1_gates_data,},
 	{.compatible = "allwinner,sun7i-a20-ahb-gates-clk", .data = &sun7i_a20_ahb_gates_data,},
 	{.compatible = "allwinner,sun4i-apb0-gates-clk", .data = &sun4i_apb0_gates_data,},
-- 
1.8.4

