From b8c666eda693906488637c414db9db35b6760e4a Mon Sep 17 00:00:00 2001
From: Daniel Schwierzeck <daniel.schwierzeck@gmail.com>
Date: Wed, 29 Aug 2012 22:08:15 +0200
Subject: net: switchlib: add driver for Lantiq PSB697X switch family

Signed-off-by: Daniel Schwierzeck <daniel.schwierzeck@gmail.com>

--- a/drivers/net/switch/Makefile
+++ b/drivers/net/switch/Makefile
@@ -11,6 +11,7 @@ include $(TOPDIR)/config.mk
 LIB	:= $(obj)libswitch.o
 
 COBJS-$(CONFIG_SWITCH_MULTI) += switch.o
+COBJS-$(CONFIG_SWITCH_PSB697X) += psb697x.o
 
 COBJS	:= $(COBJS-y)
 SRCS	:= $(COBJS:.o=.c)
--- /dev/null
+++ b/drivers/net/switch/psb697x.c
@@ -0,0 +1,119 @@
+/*
+ * Copyright (C) 2011-2012 Daniel Schwierzeck, daniel.schwierzeck@gmail.com
+ *
+ * This file is released under the terms of GPL v2 and any later version.
+ * See the file COPYING in the root directory of the source tree for details.
+ */
+
+#include <common.h>
+#include <malloc.h>
+#include <switch.h>
+#include <miiphy.h>
+
+#define PSB697X_CHIPID1		0x2599
+#define PSB697X_PORT_COUNT	7
+
+#define PSB697X_PORT_BASE(p)	(p * 0x20)
+#define PSB697X_REG_PS(p)	(PSB697X_PORT_BASE(p) + 0x00)
+#define PSB697X_REG_PBC(p)	(PSB697X_PORT_BASE(p) + 0x01)
+#define PSB697X_REG_PEC(p)	(PSB697X_PORT_BASE(p) + 0x02)
+
+#define PSB697X_REG_SGC1	0x0E0	/* Switch Global Control Register 1 */
+#define PSB697X_REG_SGC2	0x0E1	/* Switch Global Control Register 2 */
+#define PSB697X_REG_CMH		0x0E2	/* CPU Port & Mirror Control */
+#define PSB697X_REG_MIICR	0x0F5	/* MII Port Control */
+#define PSB697X_REG_CI0		0x100	/* Chip Identifier 0 */
+#define PSB697X_REG_CI1		0x101	/* Chip Identifier 1 */
+#define PSB697X_REG_MIIAC	0x120	/* MII Indirect Access Control */
+#define PSB697X_REG_MIIWD	0x121	/* MII Indirect Write Data */
+#define PSB697X_REG_MIIRD	0x122	/* MII Indirect Read Data */
+
+#define PSB697X_REG_PORT_FLP	(1 << 2)	/* Force link up */
+#define PSB697X_REG_PORT_FLD	(1 << 1)	/* Force link down */
+
+#define PSB697X_REG_SGC2_SE	(1 << 15)	/* Switch enable */
+
+#define PSB697X_REG_CMH_CPN_MASK	0x7
+#define PSB697X_REG_CMH_CPN_SHIFT	5
+
+
+static inline int psb697x_mii_read(struct mii_dev *bus, u16 reg)
+{
+	int ret;
+
+	ret = bus->read(bus, (reg >> 5) & 0x1f, MDIO_DEVAD_NONE, reg & 0x1f);
+
+	return ret;
+}
+
+static inline int psb697x_mii_write(struct mii_dev *bus, u16 reg, u16 val)
+{
+	int ret;
+
+	ret = bus->write(bus, (reg >> 5) & 0x1f, MDIO_DEVAD_NONE,
+		reg & 0x1f, val);
+
+	return ret;
+}
+
+static int psb697x_probe(struct switch_device *dev)
+{
+	struct mii_dev *bus = dev->bus;
+	int ci1;
+
+	ci1 = psb697x_mii_read(bus, PSB697X_REG_CI1);
+
+	if (ci1 == PSB697X_CHIPID1)
+		return 0;
+
+	return 1;
+}
+
+static void psb697x_setup(struct switch_device *dev)
+{
+	struct mii_dev *bus = dev->bus;
+	int i, state;
+
+	/* Enable switch */
+	psb697x_mii_write(bus, PSB697X_REG_SGC2, PSB697X_REG_SGC2_SE);
+
+	/*
+	 * Force 100 Mbps as default value for CPU ports 5 and 6 to get
+	 * full speed.
+	 */
+	psb697x_mii_write(bus, PSB697X_REG_MIICR, 0x0773);
+
+	for (i = 0; i < PSB697X_PORT_COUNT; i++) {
+		state = dev->port_mask & (1 << i);
+
+		/*
+		 * Software workaround from Errata Sheet:
+		 * Force link down and reset internal PHY, keep that state
+		 * for all unconnected ports and disable force link down
+		 * for all connected ports
+		 */
+		psb697x_mii_write(bus, PSB697X_REG_PBC(i),
+			PSB697X_REG_PORT_FLD);
+
+		if (i == dev->cpu_port)
+			/* Force link up for CPU port */
+			psb697x_mii_write(bus, PSB697X_REG_PBC(i),
+				PSB697X_REG_PORT_FLP);
+		else if (state)
+			/* Disable force link down for active LAN ports */
+			psb697x_mii_write(bus, PSB697X_REG_PBC(i), 0);
+	}
+}
+
+static struct switch_driver psb697x_drv = {
+	.name = "psb697x",
+};
+
+void switch_psb697x_init(void)
+{
+	/* For archs with manual relocation */
+	psb697x_drv.probe = psb697x_probe;
+	psb697x_drv.setup = psb697x_setup;
+
+	switch_driver_register(&psb697x_drv);
+}
--- a/drivers/net/switch/switch.c
+++ b/drivers/net/switch/switch.c
@@ -18,6 +18,10 @@ void switch_init(void)
 	INIT_LIST_HEAD(&switch_drivers);
 	INIT_LIST_HEAD(&switch_devices);
 
+#if defined(CONFIG_SWITCH_PSB697X)
+	switch_psb697x_init();
+#endif
+
 	board_switch_init();
 }
 
--- a/include/switch.h
+++ b/include/switch.h
@@ -90,6 +90,7 @@ static inline void switch_setup(struct s
 }
 
 /* Init functions for supported Switch drivers */
+extern void switch_psb697x_init(void);
 
 #endif /* __SWITCH_H */
 
