From 3e52e08e7f8f9cb1137f232e3bfa00f89ed27475 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Sat, 7 Dec 2013 12:38:32 +0100
Subject: [PATCH] ARM: sun7i: dt: Fix interrupt trigger types

The Allwinner A20 uses the ARM GIC as its internal interrupts controller. The
GIC can work on several interrupt triggers, and the A20 was actually setting it
up to use a rising edge as a trigger, while it was actually a level high
trigger, leading to some interrupts that would be completely ignored if the
edge was missed.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
Reported-by: Hans de Goede <hdegoede@redhat.com>
Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun7i-a20.dtsi | 42 ++++++++++++++++++++--------------------
 1 file changed, 21 insertions(+), 21 deletions(-)

diff --git a/arch/arm/boot/dts/sun7i-a20.dtsi b/arch/arm/boot/dts/sun7i-a20.dtsi
index f1a6b24..0b7fcc1 100644
--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -298,7 +298,7 @@
 		emac: ethernet@01c0b000 {
 			compatible = "allwinner,sun4i-emac";
 			reg = <0x01c0b000 0x1000>;
-			interrupts = <0 55 1>;
+			interrupts = <0 55 4>;
 			clocks = <&ahb_gates 17>;
 			status = "disabled";
 		};
@@ -324,7 +324,7 @@
 		pio: pinctrl@01c20800 {
 			compatible = "allwinner,sun7i-a20-pinctrl";
 			reg = <0x01c20800 0x400>;
-			interrupts = <0 28 1>;
+			interrupts = <0 28 4>;
 			clocks = <&apb0_gates 5>;
 			gpio-controller;
 			interrupt-controller;
@@ -405,12 +405,12 @@
 		timer@01c20c00 {
 			compatible = "allwinner,sun4i-timer";
 			reg = <0x01c20c00 0x90>;
-			interrupts = <0 22 1>,
-				     <0 23 1>,
-				     <0 24 1>,
-				     <0 25 1>,
-				     <0 67 1>,
-				     <0 68 1>;
+			interrupts = <0 22 4>,
+				     <0 23 4>,
+				     <0 24 4>,
+				     <0 25 4>,
+				     <0 67 4>,
+				     <0 68 4>;
 			clocks = <&osc24M>;
 		};
 
@@ -432,7 +432,7 @@
 		uart0: serial@01c28000 {
 			compatible = "snps,dw-apb-uart";
 			reg = <0x01c28000 0x400>;
-			interrupts = <0 1 1>;
+			interrupts = <0 1 4>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
 			clocks = <&apb1_gates 16>;
@@ -442,7 +442,7 @@
 		uart1: serial@01c28400 {
 			compatible = "snps,dw-apb-uart";
 			reg = <0x01c28400 0x400>;
-			interrupts = <0 2 1>;
+			interrupts = <0 2 4>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
 			clocks = <&apb1_gates 17>;
@@ -452,7 +452,7 @@
 		uart2: serial@01c28800 {
 			compatible = "snps,dw-apb-uart";
 			reg = <0x01c28800 0x400>;
-			interrupts = <0 3 1>;
+			interrupts = <0 3 4>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
 			clocks = <&apb1_gates 18>;
@@ -462,7 +462,7 @@
 		uart3: serial@01c28c00 {
 			compatible = "snps,dw-apb-uart";
 			reg = <0x01c28c00 0x400>;
-			interrupts = <0 4 1>;
+			interrupts = <0 4 4>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
 			clocks = <&apb1_gates 19>;
@@ -472,7 +472,7 @@
 		uart4: serial@01c29000 {
 			compatible = "snps,dw-apb-uart";
 			reg = <0x01c29000 0x400>;
-			interrupts = <0 17 1>;
+			interrupts = <0 17 4>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
 			clocks = <&apb1_gates 20>;
@@ -482,7 +482,7 @@
 		uart5: serial@01c29400 {
 			compatible = "snps,dw-apb-uart";
 			reg = <0x01c29400 0x400>;
-			interrupts = <0 18 1>;
+			interrupts = <0 18 4>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
 			clocks = <&apb1_gates 21>;
@@ -492,7 +492,7 @@
 		uart6: serial@01c29800 {
 			compatible = "snps,dw-apb-uart";
 			reg = <0x01c29800 0x400>;
-			interrupts = <0 19 1>;
+			interrupts = <0 19 4>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
 			clocks = <&apb1_gates 22>;
@@ -502,7 +502,7 @@
 		uart7: serial@01c29c00 {
 			compatible = "snps,dw-apb-uart";
 			reg = <0x01c29c00 0x400>;
-			interrupts = <0 20 1>;
+			interrupts = <0 20 4>;
 			reg-shift = <2>;
 			reg-io-width = <4>;
 			clocks = <&apb1_gates 23>;
@@ -512,7 +512,7 @@
 		i2c0: i2c@01c2ac00 {
 			compatible = "allwinner,sun4i-i2c";
 			reg = <0x01c2ac00 0x400>;
-			interrupts = <0 7 1>;
+			interrupts = <0 7 4>;
 			clocks = <&apb1_gates 0>;
 			clock-frequency = <100000>;
 			status = "disabled";
@@ -521,7 +521,7 @@
 		i2c1: i2c@01c2b000 {
 			compatible = "allwinner,sun4i-i2c";
 			reg = <0x01c2b000 0x400>;
-			interrupts = <0 8 1>;
+			interrupts = <0 8 4>;
 			clocks = <&apb1_gates 1>;
 			clock-frequency = <100000>;
 			status = "disabled";
@@ -530,7 +530,7 @@
 		i2c2: i2c@01c2b400 {
 			compatible = "allwinner,sun4i-i2c";
 			reg = <0x01c2b400 0x400>;
-			interrupts = <0 9 1>;
+			interrupts = <0 9 4>;
 			clocks = <&apb1_gates 2>;
 			clock-frequency = <100000>;
 			status = "disabled";
@@ -539,7 +539,7 @@
 		i2c3: i2c@01c2b800 {
 			compatible = "allwinner,sun4i-i2c";
 			reg = <0x01c2b800 0x400>;
-			interrupts = <0 88 1>;
+			interrupts = <0 88 4>;
 			clocks = <&apb1_gates 3>;
 			clock-frequency = <100000>;
 			status = "disabled";
@@ -548,7 +548,7 @@
 		i2c4: i2c@01c2bc00 {
 			compatible = "allwinner,sun4i-i2c";
 			reg = <0x01c2bc00 0x400>;
-			interrupts = <0 89 1>;
+			interrupts = <0 89 4>;
 			clocks = <&apb1_gates 15>;
 			clock-frequency = <100000>;
 			status = "disabled";
-- 
1.8.5.1

