From e8966070a22744582a2b7b63d8dab82f05499eb2 Mon Sep 17 00:00:00 2001
From: Hans de Goede <hdegoede@redhat.com>
Date: Tue, 17 Dec 2013 23:27:03 +0100
Subject: [PATCH] ARM: sunxi-ehci: Fix resource check

Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 drivers/usb/host/ehci-sunxi.c | 3 ++-
 1 file changed, 2 insertions(+), 1 deletion(-)

diff --git a/drivers/usb/host/ehci-sunxi.c b/drivers/usb/host/ehci-sunxi.c
index e7e15cc..e050d78 100644
--- a/drivers/usb/host/ehci-sunxi.c
+++ b/drivers/usb/host/ehci-sunxi.c
@@ -332,7 +332,8 @@ static int sunxi_ehci_probe(struct platform_device *pdev)
 	if (pdev->resource[0].flags != IORESOURCE_MEM
 			|| pdev->resource[1].flags != IORESOURCE_MEM
 			|| pdev->resource[2].flags != IORESOURCE_MEM
-			|| pdev->resource[3].flags != IORESOURCE_IRQ) {
+			|| (pdev->resource[3].flags & IORESOURCE_TYPE_BITS)
+				!= IORESOURCE_IRQ) {
 		dev_err(&pdev->dev, "invalid resource type\n");
 		return -ENODEV;
 	}
-- 
1.8.5.1

