--- a/drivers/mtd/bcm47xxpart.c
+++ b/drivers/mtd/bcm47xxpart.c
@@ -23,9 +23,10 @@
  * Amount of bytes we read when analyzing each block of flash memory.
  * Set it big enough to allow detecting partition and reading important data.
  */
-#define BCM47XXPART_BYTES_TO_READ	0x404
+#define BCM47XXPART_BYTES_TO_READ	0x4e8
 
 /* Magics */
+#define CFE_MAGIC			0x43464531	/* 1EFC */
 #define BOARD_DATA_MAGIC		0x5246504D	/* MPFR */
 #define POT_MAGIC1			0x54544f50	/* POTT */
 #define POT_MAGIC2			0x504f		/* OP */
@@ -93,8 +94,9 @@ static int bcm47xxpart_parse(struct mtd_
 			continue;
 		}
 
-		/* CFE has small NVRAM at 0x400 */
-		if (buf[0x400 / 4] == NVRAM_HEADER) {
+		/* Magic or small NVRAM at 0x400 */
+		if (buf[0x4e0 / 4] == CFE_MAGIC ||
+		    buf[0x400 / 4] == NVRAM_HEADER) {
 			bcm47xxpart_add_part(&parts[curr_part++], "boot",
 					     offset, MTD_WRITEABLE);
 			continue;
