From 079441036b20d9f3d23d1e96f0681b99349de05a Mon Sep 17 00:00:00 2001
From: Tim Harvey <tharvey@gateworks.com>
Date: Tue, 22 Oct 2013 21:51:28 -0700
Subject: [PATCH] imx: add PCI fixup for PEX860X on Gateworks board

The PEX860X has GPIO's which are used for PCI Reset lines on the
Gateworks Ventana boards.  The GPIO's need to be set as output
level high so as to allow the PCIe devices to come out of reset.

Signed-off-by: Tim Harvey <tharvey@gateworks.com>
Signed-off-by: Shawn Guo <shawn.guo@linaro.org>
---
 arch/arm/mach-imx/mach-imx6q.c | 30 ++++++++++++++++++++++++++++++
 1 file changed, 30 insertions(+)

--- a/arch/arm/mach-imx/mach-imx6q.c
+++ b/arch/arm/mach-imx/mach-imx6q.c
@@ -26,6 +26,7 @@
 #include <linux/of_irq.h>
 #include <linux/of_platform.h>
 #include <linux/opp.h>
+#include <linux/pci.h>
 #include <linux/phy.h>
 #include <linux/reboot.h>
 #include <linux/regmap.h>
@@ -134,6 +135,34 @@ static int ksz9031rn_phy_fixup(struct ph
 	return 0;
 }
 
+/*
+ * fixup for PLX PEX8909 bridge to configure GPIO1-7 as output High
+ * as they are used for slots1-7 PERST#
+ */
+static void ventana_pciesw_early_fixup(struct pci_dev *dev)
+{
+	u32 dw;
+
+	if (!of_machine_is_compatible("gw,ventana"))
+		return;
+
+	if (dev->devfn != 0)
+		return;
+
+	pci_read_config_dword(dev, 0x62c, &dw);
+	dw |= 0xaaa8; // GPIO1-7 outputs
+	pci_write_config_dword(dev, 0x62c, dw);
+
+	pci_read_config_dword(dev, 0x644, &dw);
+	dw |= 0xfe;   // GPIO1-7 output high
+	pci_write_config_dword(dev, 0x644, dw);
+
+	msleep(100);
+}
+DECLARE_PCI_FIXUP_EARLY(PCI_VENDOR_ID_PLX, 0x8609, ventana_pciesw_early_fixup);
+DECLARE_PCI_FIXUP_EARLY(PCI_VENDOR_ID_PLX, 0x8606, ventana_pciesw_early_fixup);
+DECLARE_PCI_FIXUP_EARLY(PCI_VENDOR_ID_PLX, 0x8604, ventana_pciesw_early_fixup);
+
 static int ar8031_phy_fixup(struct phy_device *dev)
 {
 	u16 val;
