--- a/arch/mips/bcm63xx/boards/board_bcm963xx.c
+++ b/arch/mips/bcm63xx/boards/board_bcm963xx.c
@@ -773,6 +773,60 @@ static struct board_info __initdata boar
 		},
 	},
 };
+
+// Actually this board is the very same as the rta770bw,
+// where the additional 'b' within the name just
+// just indicates 'Annex B'. The ADSL Modem itself is able
+// to handle both Annex A as well as Annex B -
+// the loaded firmware makes the only difference
+static struct board_info __initdata board_rta770w = {
+	.name				= "RTA770W",
+	.expected_cpu_id		= 0x6345,
+
+	.has_uart0			= 1,
+
+	.has_enet0			= 1,
+
+	.enet0 = {
+		.has_phy		= 1,
+		.phy_id			= 0,
+		.force_speed_100	= 1,
+		.force_duplex_full	= 1,
+	},
+
+	.leds = {
+		{
+			.name		= "RTA770W:green:usb",
+			.gpio		= 7,
+			.active_low	= 1,
+		},
+		{
+			.name		= "RTA770W:green:adsl",
+			.gpio		= 8,
+		},
+		{
+			.name		= "RTA770W:green:diag",
+			.gpio		= 10,
+			.active_low	= 1,
+		},
+		{
+			.name		= "RTA770W:green:wlan",
+			.gpio		= 11,
+			.active_low	= 1,
+		},
+	},
+
+	.buttons = {
+		{
+			.desc		= "reset",
+			.gpio		= 13,
+			.type		= EV_KEY,
+			.code		= KEY_RESTART,
+			.active_low	= 1,
+			.debounce_interval = BCM963XX_KEYS_DEBOUNCE_INTERVAL,
+		},
+	},
+};
 #endif
 
 /*
@@ -3766,6 +3820,7 @@ static const struct board_info __initcon
 #ifdef CONFIG_BCM63XX_CPU_6345
 	&board_96345gw2,
 	&board_rta770bw,
+	&board_rta770w,
 #endif
 #ifdef CONFIG_BCM63XX_CPU_6348
 	&board_96348r,
