--- a/arch/mips/bcm47xx/setup.c
+++ b/arch/mips/bcm47xx/setup.c
@@ -35,6 +35,7 @@
 #include <asm/prom.h>
 #include <asm/reboot.h>
 #include <asm/time.h>
+#include <asm/idle.h>
 #include <bcm47xx.h>
 #include <bcm47xx_nvram.h>
 #include <bcm47xx_board.h>
@@ -239,6 +240,14 @@ static int __init bcm47xx_register_bus_c
 #endif
 #ifdef CONFIG_BCM47XX_BCMA
 	case BCM47XX_BUS_TYPE_BCMA:
+		/* The BCM4706 has a problem with the CPU wait instruction.
+		 * When r4k_wait or r4k_wait_irqoff is used will just hang and 
+		 * not return from a msleep(). Removing the cpu_wait 
+		 * functionality is a workaround for this problem. The BCM4716 
+		 * does not have this problem.
+		 */
+		if (bcm47xx_bus.bcma.bus.chipinfo.id == BCMA_CHIP_ID_BCM4706)
+			cpu_wait = NULL;
 		bcma_bus_register(&bcm47xx_bus.bcma.bus);
 		break;
 #endif
