Index: linux-2.6.22-rc4/drivers/usb/host/Kconfig
===================================================================
--- linux-2.6.22-rc4.orig/drivers/usb/host/Kconfig	2007-06-10 21:32:11.000000000 +0100
+++ linux-2.6.22-rc4/drivers/usb/host/Kconfig	2007-06-10 21:33:24.000000000 +0100
@@ -142,6 +142,19 @@
 	  Enables support for PCI-bus plug-in USB controller cards.
 	  If unsure, say Y.
 
+config USB_OHCI_HCD_SSB
+	bool "OHCI support for the Broadcom SSB OHCI core (embedded systems only)"
+	depends on USB_OHCI_HCD && ((USB_OHCI_HCD=m && SSB) || (USB_OHCI_HCD=y && SSB=y)) && EXPERIMENTAL
+	default n
+	---help---
+	  Support for the Sonics Silicon Backplane (SSB) attached
+	  Broadcom USB OHCI core.
+
+	  This device is only present in some embedded devices with
+	  Broadcom based SSB bus.
+
+	  If unsure, say N.
+
 config USB_OHCI_BIG_ENDIAN_DESC
 	bool
 	depends on USB_OHCI_HCD
Index: linux-2.6.22-rc4/drivers/usb/host/ohci-hcd.c
===================================================================
--- linux-2.6.22-rc4.orig/drivers/usb/host/ohci-hcd.c	2007-06-10 21:32:11.000000000 +0100
+++ linux-2.6.22-rc4/drivers/usb/host/ohci-hcd.c	2007-06-10 21:33:24.000000000 +0100
@@ -920,11 +920,17 @@
 #define PS3_SYSTEM_BUS_DRIVER	ps3_ohci_sb_driver
 #endif
 
+#ifdef CONFIG_USB_OHCI_HCD_SSB
+#include "ohci-ssb.c"
+#define SSB_OHCI_DRIVER		ssb_ohci_driver
+#endif
+
 #if	!defined(PCI_DRIVER) &&		\
 	!defined(PLATFORM_DRIVER) &&	\
 	!defined(OF_PLATFORM_DRIVER) &&	\
 	!defined(SA1111_DRIVER) &&	\
-	!defined(PS3_SYSTEM_BUS_DRIVER)
+	!defined(PS3_SYSTEM_BUS_DRIVER) && \
+	!defined(SSB_OHCI_DRIVER)
 #error "missing bus glue for ohci-hcd"
 #endif
 
@@ -972,10 +978,20 @@
 		goto error_pci;
 #endif
 
+#ifdef SSB_OHCI_DRIVER
+	retval = ssb_driver_register(&SSB_OHCI_DRIVER);
+	if (retval)
+		goto error_ssb;
+#endif
+
 	return retval;
 
 	/* Error path */
+#ifdef SSB_OHCI_DRIVER
+ error_ssb:
+#endif
 #ifdef PCI_DRIVER
+	pci_unregister_driver(&PCI_DRIVER);
  error_pci:
 #endif
 #ifdef SA1111_DRIVER
@@ -1001,6 +1017,9 @@
 
 static void __exit ohci_hcd_mod_exit(void)
 {
+#ifdef SSB_OHCI_DRIVER
+	ssb_driver_unregister(&SSB_OHCI_DRIVER);
+#endif
 #ifdef PCI_DRIVER
 	pci_unregister_driver(&PCI_DRIVER);
 #endif
