diff -Nru linux-2.6.19.2/drivers/mtd/Kconfig linux-ar7/drivers/mtd/Kconfig
--- linux-2.6.19.2/drivers/mtd/Kconfig	2006-12-12 02:32:53.000000000 +0700
+++ linux-ar7/drivers/mtd/Kconfig	2007-02-03 22:47:10.000000000 +0700
@@ -152,6 +152,12 @@
 	  for your particular device. It won't happen automatically. The
 	  'armflash' map driver (CONFIG_MTD_ARMFLASH) does this, for example.
 
+config MTD_AR7_PARTS
+	tristate "TI AR7 partitioning support"
+	depends on MTD_PARTITIONS
+	---help---
+	  TI AR7 partitioning support
+
 comment "User Modules And Translation Layers"
 	depends on MTD
 
diff -Nru linux-2.6.19.2/drivers/mtd/Makefile linux-ar7/drivers/mtd/Makefile
--- linux-2.6.19.2/drivers/mtd/Makefile	2006-12-12 02:32:53.000000000 +0700
+++ linux-ar7/drivers/mtd/Makefile	2007-02-03 22:02:27.000000000 +0700
@@ -12,6 +12,7 @@
 obj-$(CONFIG_MTD_REDBOOT_PARTS) += redboot.o
 obj-$(CONFIG_MTD_CMDLINE_PARTS) += cmdlinepart.o
 obj-$(CONFIG_MTD_AFS_PARTS)	+= afs.o
+obj-$(CONFIG_MTD_AR7_PARTS)	+= ar7part.o
 
 # 'Users' - code which presents functionality to userspace.
 obj-$(CONFIG_MTD_CHAR)		+= mtdchar.o
diff -Nru linux-2.6.19.2/drivers/mtd/maps/physmap.c linux-ar7/drivers/mtd/maps/physmap.c
--- linux-2.6.19.2/drivers/mtd/maps/physmap.c	2006-12-12 02:32:53.000000000 +0700
+++ linux-ar7/drivers/mtd/maps/physmap.c	2007-02-03 21:57:11.000000000 +0700
@@ -74,7 +74,7 @@
 
 static const char *rom_probe_types[] = { "cfi_probe", "jedec_probe", "map_rom", NULL };
 #ifdef CONFIG_MTD_PARTITIONS
-static const char *part_probe_types[] = { "cmdlinepart", "RedBoot", NULL };
+static const char *part_probe_types[] = { "cmdlinepart", "RedBoot", "ar7part", NULL };
 #endif
 
 static int physmap_flash_probe(struct platform_device *dev)
