From 9403f1d54598ae56386a8bf47a5b6b34c884e4f5 Mon Sep 17 00:00:00 2001
From: "SkyLake.Huang" <skylake.huang@mediatek.com>
Date: Mon, 1 Jul 2024 18:54:10 +0800
Subject: [PATCH 06/13] net: phy: mediatek: Hook LED helper functions in
 mtk-ge.c

We have mtk-phy-lib.c now so that we can use LED helper functions in
mtk-ge.c(mt7531 part). It also means that mt7531/mt7981/mt7988's
Giga ethernet phys share almost the same HW LED controller design.
Also, add probe function for mt7531 so that it can initialize LED state.

Signed-off-by: SkyLake.Huang <skylake.huang@mediatek.com>
---
 drivers/net/phy/mediatek/mtk-ge.c | 100 ++++++++++++++++++++++++++++++
 1 file changed, 100 insertions(+)

--- a/drivers/net/phy/mediatek/mtk-ge.c
+++ b/drivers/net/phy/mediatek/mtk-ge.c
@@ -14,6 +14,10 @@
 #define MTK_PHY_PAGE_EXTENDED_2A30	0x2a30
 #define MTK_PHY_PAGE_EXTENDED_52B5	0x52b5
 
+struct mtk_gephy_priv {
+	unsigned long		led_state;
+};
+
 static void mtk_gephy_config_init(struct phy_device *phydev)
 {
 	/* Disable EEE */
@@ -94,6 +98,96 @@ static int mt7531_phy_config_init(struct
 	return 0;
 }
 
+static int mt7531_phy_probe(struct phy_device *phydev)
+{
+	struct mtk_gephy_priv *priv;
+
+	priv = devm_kzalloc(&phydev->mdio.dev, sizeof(struct mtk_gephy_priv),
+			    GFP_KERNEL);
+	if (!priv)
+		return -ENOMEM;
+
+	phydev->priv = priv;
+
+	mtk_phy_leds_state_init(phydev);
+
+	return 0;
+}
+
+static int mt753x_phy_led_blink_set(struct phy_device *phydev, u8 index,
+				    unsigned long *delay_on,
+				    unsigned long *delay_off)
+{
+	struct mtk_gephy_priv *priv = phydev->priv;
+	bool blinking = false;
+	int err = 0;
+
+	err = mtk_phy_led_num_dly_cfg(index, delay_on, delay_off, &blinking);
+	if (err < 0)
+		return err;
+
+	err = mtk_phy_hw_led_blink_set(phydev, index, &priv->led_state,
+				       blinking);
+	if (err)
+		return err;
+
+	return mtk_phy_hw_led_on_set(phydev, index, &priv->led_state,
+				     MTK_GPHY_LED_ON_MASK, false);
+}
+
+static int mt753x_phy_led_brightness_set(struct phy_device *phydev,
+					 u8 index, enum led_brightness value)
+{
+	struct mtk_gephy_priv *priv = phydev->priv;
+	int err;
+
+	err = mtk_phy_hw_led_blink_set(phydev, index, &priv->led_state, false);
+	if (err)
+		return err;
+
+	return mtk_phy_hw_led_on_set(phydev, index, &priv->led_state,
+				     MTK_GPHY_LED_ON_MASK, (value != LED_OFF));
+}
+
+static const unsigned long supported_triggers =
+	(BIT(TRIGGER_NETDEV_FULL_DUPLEX) |
+	 BIT(TRIGGER_NETDEV_HALF_DUPLEX) |
+	 BIT(TRIGGER_NETDEV_LINK)        |
+	 BIT(TRIGGER_NETDEV_LINK_10)     |
+	 BIT(TRIGGER_NETDEV_LINK_100)    |
+	 BIT(TRIGGER_NETDEV_LINK_1000)   |
+	 BIT(TRIGGER_NETDEV_RX)          |
+	 BIT(TRIGGER_NETDEV_TX));
+
+static int mt753x_phy_led_hw_is_supported(struct phy_device *phydev, u8 index,
+					  unsigned long rules)
+{
+	return mtk_phy_led_hw_is_supported(phydev, index, rules,
+					   supported_triggers);
+}
+
+static int mt753x_phy_led_hw_control_get(struct phy_device *phydev, u8 index,
+					 unsigned long *rules)
+{
+	struct mtk_gephy_priv *priv = phydev->priv;
+
+	return mtk_phy_led_hw_ctrl_get(phydev, index, rules, &priv->led_state,
+				       MTK_GPHY_LED_ON_SET,
+				       MTK_GPHY_LED_RX_BLINK_SET,
+				       MTK_GPHY_LED_TX_BLINK_SET);
+};
+
+static int mt753x_phy_led_hw_control_set(struct phy_device *phydev, u8 index,
+					 unsigned long rules)
+{
+	struct mtk_gephy_priv *priv = phydev->priv;
+
+	return mtk_phy_led_hw_ctrl_set(phydev, index, rules, &priv->led_state,
+				       MTK_GPHY_LED_ON_SET,
+				       MTK_GPHY_LED_RX_BLINK_SET,
+				       MTK_GPHY_LED_TX_BLINK_SET);
+};
+
 static struct phy_driver mtk_gephy_driver[] = {
 	{
 		PHY_ID_MATCH_EXACT(0x03a29412),
@@ -112,6 +206,7 @@ static struct phy_driver mtk_gephy_drive
 	{
 		PHY_ID_MATCH_EXACT(0x03a29441),
 		.name		= "MediaTek MT7531 PHY",
+		.probe		= mt7531_phy_probe,
 		.config_init	= mt7531_phy_config_init,
 		/* Interrupts are handled by the switch, not the PHY
 		 * itself.
@@ -122,6 +217,11 @@ static struct phy_driver mtk_gephy_drive
 		.resume		= genphy_resume,
 		.read_page	= mtk_phy_read_page,
 		.write_page	= mtk_phy_write_page,
+		.led_blink_set	= mt753x_phy_led_blink_set,
+		.led_brightness_set = mt753x_phy_led_brightness_set,
+		.led_hw_is_supported = mt753x_phy_led_hw_is_supported,
+		.led_hw_control_set = mt753x_phy_led_hw_control_set,
+		.led_hw_control_get = mt753x_phy_led_hw_control_get,
 	},
 };
 
