// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qca955x.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	aliases {
		label-mac-device = &eth0;
		led-boot = &led_status;
		led-failsafe = &led_status;
		led-upgrade = &led_status;
	};

	leds {
		compatible = "gpio-leds";

		led-0 {
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_WLAN;
			function-enumerator = <24>;
			linux,default-trigger = "phy1tpt";
		};

		led_status: led-1 {
			gpios = <&gpio 14 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_STATUS;
		};

		led-2 {
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_USB;
			trigger-sources = <&usb_port1>;
			linux,default-trigger = "usbport";
		};
	};

	keys {
		compatible = "gpio-keys";

		button-wps {
			label = "wps";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
			debounce-interval = <60>;
		};

		button-reset {
			label = "reset";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
			debounce-interval = <60>;
		};

		button-eject {
			label = "eject";
			gpios = <&gpio 19 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_EJECTCD>;
			debounce-interval = <60>;
		};
	};

	beeper {
		compatible = "gpio-beeper";
		gpios = <&gpio 4 GPIO_ACTIVE_HIGH>;
	};

	reg_usb_vbus: regulator {
		compatible = "regulator-fixed";
		regulator-name = "usb-vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		gpios = <&gpio 11 GPIO_ACTIVE_HIGH>;
		enable-active-high;
		regulator-always-on;
	};

	watchdog {
		compatible = "linux,wdt-gpio";
		gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		hw_algo = "toggle";
		hw_margin_ms = <300>;
		always-running;
	};
};

&mdio0 {
	status = "okay";

	ethphy4: ethernet-phy@4 {
		compatible = "ethernet-phy-id004d,d072",
			     "ethernet-phy-ieee802.3-c22";
		reg = <0x4>;
		eee-broken-100tx;
		eee-broken-1000t;
	};
};

&eth0 {
	status = "okay";

	phy-handle = <&ethphy4>;
	phy-mode = "rgmii-rxid";
	pll-data = <0xae000000 0x80000101 0x80001313>;

	nvmem-cells = <&macaddr_uboot_ethaddr 0>;
	nvmem-cell-names = "mac-address";

	gmac-config {
		device = <&gmac>;

		rxdv-delay = <3>;
		rxd-delay = <3>;
		txen-delay = <0>;
		txd-delay = <0>;
		rgmii-enabled = <1>;
	};
};

&mdio1 {
	status = "okay";

	ethphy1: ethernet-phy@1 {
		compatible = "ethernet-phy-id004d,d074",
			     "ethernet-phy-ieee802.3-c22";
		reg = <0x1>;
		at803x-override-sgmii-link-check;
	};
};

&eth1 {
	status = "okay";

	phy-handle = <&ethphy1>;
	pll-data = <0x03000000 0x00000101 0x00001313>;

	qca955x-sgmii-fixup;
};

&pcie0 {
	status = "okay";

	wifi@0,0 {
		compatible = "qcom,ath10k";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&cal_art_5000>, <&macaddr_uboot_ethaddr 1>;
		nvmem-cell-names = "calibration", "mac-address";
	};
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x40000>;
				read-only;
			};

			partition@40000 {
				compatible = "u-boot,env";
				label = "u-boot-env";
				reg = <0x40000 0x10000>;
				read-only;

				macaddr_uboot_ethaddr: ethaddr {
					#nvmem-cell-cells = <1>;
				};
			};

			partition@50000 {
				label = "art";
				reg = <0x50000 0x10000>;
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					cal_art_1000: calibration@1000 {
						reg = <0x1000 0x440>;
					};

					cal_art_5000: calibration@5000 {
						reg = <0x5000 0x844>;
					};
				};
			};

			partition@60000 {
				label = "art2";
				reg = <0x60000 0x10000>;
				read-only;
			};

			partition@70000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x70000 0xe00000>;
			};

			partition@e70000 {
				label = "manufacture";
				reg = <0xe70000 0x100000>;
				read-only;
			};

			partition@f70000 {
				label = "backup";
				reg = <0xf70000 0x10000>;
				read-only;
			};

			partition@f80000 {
				label = "storage";
				reg = <0xf80000 0x80000>;
				read-only;
			};
		};
	};
};

&usb_phy0 {
	status = "okay";
};

&usb0 {
	#address-cells = <1>;
	#size-cells = <0>;
	status = "okay";

	dr_mode = "host";
	vbus-supply = <&reg_usb_vbus>;

	usb_port1: port@1 {
		reg = <1>;
		#trigger-source-cells = <0>;
	};
};

&wdt {
	status = "disabled";
};

&wmac {
	status = "okay";

	nvmem-cells = <&cal_art_1000>, <&macaddr_uboot_ethaddr 0>;
	nvmem-cell-names = "calibration", "mac-address";
};
