From 76c345edef754b16cab81ad9452cc49c09e67066 Mon Sep 17 00:00:00 2001
From: Chen-Yu Tsai <wenst@chromium.org>
Date: Sat, 24 Feb 2024 11:45:14 +0000
Subject: [PATCH] nvmem: mtk-efuse: Drop NVMEM device name
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

The MT8183 has not one but two efuse devices. The static name and ID
causes the second efuse device to fail to probe, due to duplicate sysfs
entries.

With the rework of the mtk-socinfo driver, lookup by name is no longer
necessary. The custom name can simply be dropped.

Signed-off-by: Chen-Yu Tsai <wenst@chromium.org>
Reviewed-by: AngeloGioacchino Del Regno <angelogioacchino.delregno@collabora.com>
Tested-by: "Nícolas F. R. A. Prado" <nfraprado@collabora.com>
Signed-off-by: Srinivas Kandagatla <srinivas.kandagatla@linaro.org>
Link: https://lore.kernel.org/r/20240224114516.86365-10-srinivas.kandagatla@linaro.org
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/nvmem/mtk-efuse.c | 1 -
 1 file changed, 1 deletion(-)

--- a/drivers/nvmem/mtk-efuse.c
+++ b/drivers/nvmem/mtk-efuse.c
@@ -86,7 +86,6 @@ static int mtk_efuse_probe(struct platfo
 	econfig.size = resource_size(res);
 	econfig.priv = priv;
 	econfig.dev = dev;
-	econfig.name = "mtk-efuse";
 	if (pdata->uses_post_processing)
 		econfig.fixup_dt_cell_info = &mtk_efuse_fixup_dt_cell_info;
 	nvmem = devm_nvmem_register(dev, &econfig);
