From e73df692396b0d6bdcb2317299fa1e8e547f3446 Mon Sep 17 00:00:00 2001
From: "SkyLake.Huang" <skylake.huang@mediatek.com>
Date: Mon, 1 Jul 2024 18:54:12 +0800
Subject: [PATCH 08/13] net: phy: mediatek: Change mtk-ge-soc.c line wrapping

This patch shrinks mtk-ge-soc.c line wrapping to 80 characters.

Signed-off-by: SkyLake.Huang <skylake.huang@mediatek.com>
---
 drivers/net/phy/mediatek/mtk-ge-soc.c | 67 +++++++++++++++++----------
 1 file changed, 42 insertions(+), 25 deletions(-)

--- a/drivers/net/phy/mediatek/mtk-ge-soc.c
+++ b/drivers/net/phy/mediatek/mtk-ge-soc.c
@@ -295,7 +295,8 @@ static int cal_cycle(struct phy_device *
 	ret = phy_read_mmd_poll_timeout(phydev, MDIO_MMD_VEND1,
 					MTK_PHY_RG_AD_CAL_CLK, reg_val,
 					reg_val & MTK_PHY_DA_CAL_CLK, 500,
-					ANALOG_INTERNAL_OPERATION_MAX_US, false);
+					ANALOG_INTERNAL_OPERATION_MAX_US,
+					false);
 	if (ret) {
 		phydev_err(phydev, "Calibration cycle timeout\n");
 		return ret;
@@ -304,7 +305,7 @@ static int cal_cycle(struct phy_device *
 	phy_clear_bits_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_AD_CALIN,
 			   MTK_PHY_DA_CALIN_FLAG);
 	ret = phy_read_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_AD_CAL_COMP) >>
-			   MTK_PHY_AD_CAL_COMP_OUT_SHIFT;
+	      MTK_PHY_AD_CAL_COMP_OUT_SHIFT;
 	phydev_dbg(phydev, "cal_val: 0x%x, ret: %d\n", cal_val, ret);
 
 	return ret;
@@ -394,38 +395,46 @@ static int tx_amp_fill_result(struct phy
 	}
 
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TXVLD_DA_RG,
-		       MTK_PHY_DA_TX_I2MPB_A_GBE_MASK, (buf[0] + bias[0]) << 10);
+		       MTK_PHY_DA_TX_I2MPB_A_GBE_MASK,
+		       (buf[0] + bias[0]) << 10);
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TXVLD_DA_RG,
 		       MTK_PHY_DA_TX_I2MPB_A_TBT_MASK, buf[0] + bias[1]);
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_A2,
-		       MTK_PHY_DA_TX_I2MPB_A_HBT_MASK, (buf[0] + bias[2]) << 10);
+		       MTK_PHY_DA_TX_I2MPB_A_HBT_MASK,
+		       (buf[0] + bias[2]) << 10);
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_A2,
 		       MTK_PHY_DA_TX_I2MPB_A_TST_MASK, buf[0] + bias[3]);
 
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_B1,
-		       MTK_PHY_DA_TX_I2MPB_B_GBE_MASK, (buf[1] + bias[4]) << 8);
+		       MTK_PHY_DA_TX_I2MPB_B_GBE_MASK,
+		       (buf[1] + bias[4]) << 8);
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_B1,
 		       MTK_PHY_DA_TX_I2MPB_B_TBT_MASK, buf[1] + bias[5]);
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_B2,
-		       MTK_PHY_DA_TX_I2MPB_B_HBT_MASK, (buf[1] + bias[6]) << 8);
+		       MTK_PHY_DA_TX_I2MPB_B_HBT_MASK,
+		       (buf[1] + bias[6]) << 8);
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_B2,
 		       MTK_PHY_DA_TX_I2MPB_B_TST_MASK, buf[1] + bias[7]);
 
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_C1,
-		       MTK_PHY_DA_TX_I2MPB_C_GBE_MASK, (buf[2] + bias[8]) << 8);
+		       MTK_PHY_DA_TX_I2MPB_C_GBE_MASK,
+		       (buf[2] + bias[8]) << 8);
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_C1,
 		       MTK_PHY_DA_TX_I2MPB_C_TBT_MASK, buf[2] + bias[9]);
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_C2,
-		       MTK_PHY_DA_TX_I2MPB_C_HBT_MASK, (buf[2] + bias[10]) << 8);
+		       MTK_PHY_DA_TX_I2MPB_C_HBT_MASK,
+		       (buf[2] + bias[10]) << 8);
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_C2,
 		       MTK_PHY_DA_TX_I2MPB_C_TST_MASK, buf[2] + bias[11]);
 
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_D1,
-		       MTK_PHY_DA_TX_I2MPB_D_GBE_MASK, (buf[3] + bias[12]) << 8);
+		       MTK_PHY_DA_TX_I2MPB_D_GBE_MASK,
+		       (buf[3] + bias[12]) << 8);
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_D1,
 		       MTK_PHY_DA_TX_I2MPB_D_TBT_MASK, buf[3] + bias[13]);
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_D2,
-		       MTK_PHY_DA_TX_I2MPB_D_HBT_MASK, (buf[3] + bias[14]) << 8);
+		       MTK_PHY_DA_TX_I2MPB_D_HBT_MASK,
+		       (buf[3] + bias[14]) << 8);
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_TX_I2MPB_TEST_MODE_D2,
 		       MTK_PHY_DA_TX_I2MPB_D_TST_MASK, buf[3] + bias[15]);
 
@@ -616,7 +625,8 @@ static int tx_vcm_cal_sw(struct phy_devi
 		goto restore;
 
 	/* We calibrate TX-VCM in different logic. Check upper index and then
-	 * lower index. If this calibration is valid, apply lower index's result.
+	 * lower index. If this calibration is valid, apply lower index's
+	 * result.
 	 */
 	ret = upper_ret - lower_ret;
 	if (ret == 1) {
@@ -645,7 +655,8 @@ static int tx_vcm_cal_sw(struct phy_devi
 	} else if (upper_idx == TXRESERVE_MAX && upper_ret == 0 &&
 		   lower_ret == 0) {
 		ret = 0;
-		phydev_warn(phydev, "TX-VCM SW cal result at high margin 0x%x\n",
+		phydev_warn(phydev,
+			    "TX-VCM SW cal result at high margin 0x%x\n",
 			    upper_idx);
 	} else {
 		ret = -EINVAL;
@@ -749,7 +760,8 @@ static void mt7981_phy_finetune(struct p
 
 	/* TR_OPEN_LOOP_EN = 1, lpf_x_average = 9 */
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG234,
-		       MTK_PHY_TR_OPEN_LOOP_EN_MASK | MTK_PHY_LPF_X_AVERAGE_MASK,
+		       MTK_PHY_TR_OPEN_LOOP_EN_MASK |
+		       MTK_PHY_LPF_X_AVERAGE_MASK,
 		       BIT(0) | FIELD_PREP(MTK_PHY_LPF_X_AVERAGE_MASK, 0x9));
 
 	/* rg_tr_lpf_cnt_val = 512 */
@@ -818,7 +830,8 @@ static void mt7988_phy_finetune(struct p
 
 	/* TR_OPEN_LOOP_EN = 1, lpf_x_average = 10 */
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1, MTK_PHY_RG_DEV1E_REG234,
-		       MTK_PHY_TR_OPEN_LOOP_EN_MASK | MTK_PHY_LPF_X_AVERAGE_MASK,
+		       MTK_PHY_TR_OPEN_LOOP_EN_MASK |
+		       MTK_PHY_LPF_X_AVERAGE_MASK,
 		       BIT(0) | FIELD_PREP(MTK_PHY_LPF_X_AVERAGE_MASK, 0xa));
 
 	/* rg_tr_lpf_cnt_val = 1023 */
@@ -930,7 +943,8 @@ static void mt798x_phy_eee(struct phy_de
 	phy_restore_page(phydev, MTK_PHY_PAGE_STANDARD, 0);
 
 	phy_select_page(phydev, MTK_PHY_PAGE_EXTENDED_3);
-	__phy_modify(phydev, MTK_PHY_LPI_REG_14, MTK_PHY_LPI_WAKE_TIMER_1000_MASK,
+	__phy_modify(phydev, MTK_PHY_LPI_REG_14,
+		     MTK_PHY_LPI_WAKE_TIMER_1000_MASK,
 		     FIELD_PREP(MTK_PHY_LPI_WAKE_TIMER_1000_MASK, 0x19c));
 
 	__phy_modify(phydev, MTK_PHY_LPI_REG_1c, MTK_PHY_SMI_DET_ON_THRESH_MASK,
@@ -940,7 +954,8 @@ static void mt798x_phy_eee(struct phy_de
 	phy_modify_mmd(phydev, MDIO_MMD_VEND1,
 		       MTK_PHY_RG_LPI_PCS_DSP_CTRL_REG122,
 		       MTK_PHY_LPI_NORM_MSE_HI_THRESH1000_MASK,
-		       FIELD_PREP(MTK_PHY_LPI_NORM_MSE_HI_THRESH1000_MASK, 0xff));
+		       FIELD_PREP(MTK_PHY_LPI_NORM_MSE_HI_THRESH1000_MASK,
+				  0xff));
 }
 
 static int cal_sw(struct phy_device *phydev, enum CAL_ITEM cal_item,
@@ -1119,14 +1134,15 @@ static int mt798x_phy_led_brightness_set
 				     MTK_GPHY_LED_ON_MASK, (value != LED_OFF));
 }
 
-static const unsigned long supported_triggers = (BIT(TRIGGER_NETDEV_FULL_DUPLEX) |
-						 BIT(TRIGGER_NETDEV_HALF_DUPLEX) |
-						 BIT(TRIGGER_NETDEV_LINK)        |
-						 BIT(TRIGGER_NETDEV_LINK_10)     |
-						 BIT(TRIGGER_NETDEV_LINK_100)    |
-						 BIT(TRIGGER_NETDEV_LINK_1000)   |
-						 BIT(TRIGGER_NETDEV_RX)          |
-						 BIT(TRIGGER_NETDEV_TX));
+static const unsigned long supported_triggers =
+	(BIT(TRIGGER_NETDEV_FULL_DUPLEX) |
+	 BIT(TRIGGER_NETDEV_HALF_DUPLEX) |
+	 BIT(TRIGGER_NETDEV_LINK)        |
+	 BIT(TRIGGER_NETDEV_LINK_10)     |
+	 BIT(TRIGGER_NETDEV_LINK_100)    |
+	 BIT(TRIGGER_NETDEV_LINK_1000)   |
+	 BIT(TRIGGER_NETDEV_RX)          |
+	 BIT(TRIGGER_NETDEV_TX));
 
 static int mt798x_phy_led_hw_is_supported(struct phy_device *phydev, u8 index,
 					  unsigned long rules)
@@ -1189,7 +1205,8 @@ static int mt7988_phy_fix_leds_polaritie
 	/* Only now setup pinctrl to avoid bogus blinking */
 	pinctrl = devm_pinctrl_get_select(&phydev->mdio.dev, "gbe-led");
 	if (IS_ERR(pinctrl))
-		dev_err(&phydev->mdio.bus->dev, "Failed to setup PHY LED pinctrl\n");
+		dev_err(&phydev->mdio.bus->dev,
+			"Failed to setup PHY LED pinctrl\n");
 
 	return 0;
 }
