From a9544caa482a7ed215117a902f04185216997831 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ar=C4=B1n=C3=A7=20=C3=9CNAL?= <arinc.unal@arinc9.com>
Date: Fri, 1 Mar 2024 12:43:04 +0200
Subject: [PATCH 44/48] net: dsa: mt7530: sort link settings ops and force link
 down on all ports
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

port_enable and port_disable clears the link settings. Move that to
mt7530_setup() and mt7531_setup_common() which set up the switches. This
way, the link settings are cleared on all ports at setup, and then only
once with phylink_mac_link_down() when a link goes down.

Enable force mode at setup to apply the force part of the link settings.
This ensures that disabled ports will have their link down.

Suggested-by: Vladimir Oltean <olteanv@gmail.com>
Signed-off-by: Arınç ÜNAL <arinc.unal@arinc9.com>
Signed-off-by: Paolo Abeni <pabeni@redhat.com>
---
 drivers/net/dsa/mt7530.c | 14 ++++++++++++--
 1 file changed, 12 insertions(+), 2 deletions(-)

--- a/drivers/net/dsa/mt7530.c
+++ b/drivers/net/dsa/mt7530.c
@@ -1222,7 +1222,6 @@ mt7530_port_enable(struct dsa_switch *ds
 	priv->ports[port].enable = true;
 	mt7530_rmw(priv, MT7530_PCR_P(port), PCR_MATRIX_MASK,
 		   priv->ports[port].pm);
-	mt7530_clear(priv, MT7530_PMCR_P(port), PMCR_LINK_SETTINGS_MASK);
 
 	mutex_unlock(&priv->reg_mutex);
 
@@ -1242,7 +1241,6 @@ mt7530_port_disable(struct dsa_switch *d
 	priv->ports[port].enable = false;
 	mt7530_rmw(priv, MT7530_PCR_P(port), PCR_MATRIX_MASK,
 		   PCR_MATRIX_CLR);
-	mt7530_clear(priv, MT7530_PMCR_P(port), PMCR_LINK_SETTINGS_MASK);
 
 	mutex_unlock(&priv->reg_mutex);
 }
@@ -2460,6 +2458,12 @@ mt7530_setup(struct dsa_switch *ds)
 	mt7530_mib_reset(ds);
 
 	for (i = 0; i < MT7530_NUM_PORTS; i++) {
+		/* Clear link settings and enable force mode to force link down
+		 * on all ports until they're enabled later.
+		 */
+		mt7530_rmw(priv, MT7530_PMCR_P(i), PMCR_LINK_SETTINGS_MASK |
+			   PMCR_FORCE_MODE, PMCR_FORCE_MODE);
+
 		/* Disable forwarding by default on all ports */
 		mt7530_rmw(priv, MT7530_PCR_P(i), PCR_MATRIX_MASK,
 			   PCR_MATRIX_CLR);
@@ -2565,6 +2569,12 @@ mt7531_setup_common(struct dsa_switch *d
 		     UNU_FFP_MASK);
 
 	for (i = 0; i < MT7530_NUM_PORTS; i++) {
+		/* Clear link settings and enable force mode to force link down
+		 * on all ports until they're enabled later.
+		 */
+		mt7530_rmw(priv, MT7530_PMCR_P(i), PMCR_LINK_SETTINGS_MASK |
+			   MT7531_FORCE_MODE, MT7531_FORCE_MODE);
+
 		/* Disable forwarding by default on all ports */
 		mt7530_rmw(priv, MT7530_PCR_P(i), PCR_MATRIX_MASK,
 			   PCR_MATRIX_CLR);
