From 39f59c72ad3a1eaab9a60f0671bc94d2bc826d21 Mon Sep 17 00:00:00 2001
From: Heiner Kallweit <hkallweit1@gmail.com>
Date: Sun, 7 Apr 2024 23:19:25 +0200
Subject: [PATCH] r8169: add support for RTL8168M
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

A user reported an unknown chip version. According to the r8168 vendor
driver it's called RTL8168M, but handling is identical to RTL8168H.
So let's simply treat it as RTL8168H.

Tested-by: Евгений <octobergun@gmail.com>
Signed-off-by: Heiner Kallweit <hkallweit1@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/ethernet/realtek/r8169_main.c | 2 ++
 1 file changed, 2 insertions(+)

--- a/drivers/net/ethernet/realtek/r8169_main.c
+++ b/drivers/net/ethernet/realtek/r8169_main.c
@@ -2230,6 +2230,8 @@ static enum mac_version rtl8169_get_mac_
 		 * the wild. Let's disable detection.
 		 * { 0x7cf, 0x540,	RTL_GIGA_MAC_VER_45 },
 		 */
+		/* Realtek calls it RTL8168M, but it's handled like RTL8168H */
+		{ 0x7cf, 0x6c0,	RTL_GIGA_MAC_VER_46 },
 
 		/* 8168G family. */
 		{ 0x7cf, 0x5c8,	RTL_GIGA_MAC_VER_44 },
