From 0de82310d2b32e78ff79d42c08b1122a6ede3778 Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Sun, 30 Apr 2023 00:15:41 +0100
Subject: [PATCH] net: phy: realtek: detect early version of RTL8221B

Early versions (?) of the RTL8221B PHY cannot be identified in a regular
Clause-45 bus scan as the PHY doesn't report the implemented MMDs
correctly but returns 0 instead.
Implement custom identify function using the PKGID instead of iterating
over the implemented MMDs.

Signed-off-by: Daniel Golle <daniel@makrotopia.org>

--- a/drivers/net/phy/realtek.c
+++ b/drivers/net/phy/realtek.c
@@ -79,6 +79,7 @@
 #define RTLGEN_SPEED_MASK			0x0630
 
 #define RTL_GENERIC_PHYID			0x001cc800
+#define RTL_8221B_VB_CG_PHYID			0x001cc849
 
 MODULE_DESCRIPTION("Realtek PHY driver");
 MODULE_AUTHOR("Johnson Leung");
@@ -744,6 +745,38 @@ static int rtl8226_match_phy_device(stru
 	       rtlgen_supports_2_5gbps(phydev);
 }
 
+static int rtl8221b_vb_cg_match_phy_device(struct phy_device *phydev)
+{
+	int val;
+	u32 id;
+
+	if (phydev->mdio.bus->probe_capabilities >= MDIOBUS_C45) {
+		val = phy_read_mmd(phydev, MDIO_MMD_PMAPMD, MDIO_PKGID1);
+		if (val < 0)
+			return 0;
+
+		id = val << 16;
+		val = phy_read_mmd(phydev, MDIO_MMD_PMAPMD, MDIO_PKGID2);
+		if (val < 0)
+			return 0;
+
+		id |= val;
+	} else {
+		val = phy_read(phydev, MII_PHYSID1);
+		if (val < 0)
+			return 0;
+
+		id = val << 16;
+		val = phy_read(phydev, MII_PHYSID2);
+		if (val < 0)
+			return 0;
+
+		id |= val;
+	}
+
+	return (id == RTL_8221B_VB_CG_PHYID);
+}
+
 static int rtl822x_probe(struct phy_device *phydev)
 {
 	struct device *dev = &phydev->mdio.dev;
@@ -1082,7 +1115,7 @@ static struct phy_driver realtek_drvs[]
 		.write_page     = rtl821x_write_page,
 		.soft_reset     = genphy_soft_reset,
 	}, {
-		PHY_ID_MATCH_EXACT(0x001cc849),
+		.match_phy_device = rtl8221b_vb_cg_match_phy_device,
 		.name           = "RTL8221B-VB-CG 2.5Gbps PHY",
 		.get_features   = rtl822x_get_features,
 		.config_init    = rtl8221b_config_init,
