From b223feb9de2a65c533ff95c08e834fa732906ea5 Mon Sep 17 00:00:00 2001
From: Eric Dumazet <edumazet@google.com>
Date: Sat, 3 Dec 2016 11:14:52 -0800
Subject: [PATCH 03/10] tcp: tsq: add shortcut in tcp_tasklet_func()

Under high stress, I've seen tcp_tasklet_func() consuming
~700 usec, handling ~150 tcp sockets.

By setting TCP_TSQ_DEFERRED in tcp_wfree(), we give a chance
for other cpus/threads entering tcp_write_xmit() to grab it,
allowing tcp_tasklet_func() to skip sockets that already did
an xmit cycle.

In the future, we might give to ACK processing an increased
budget to reduce even more tcp_tasklet_func() amount of work.

Signed-off-by: Eric Dumazet <edumazet@google.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 net/ipv4/tcp_output.c | 22 ++++++++++++----------
 1 file changed, 12 insertions(+), 10 deletions(-)

--- a/net/ipv4/tcp_output.c
+++ b/net/ipv4/tcp_output.c
@@ -767,19 +767,19 @@ static void tcp_tasklet_func(unsigned lo
 	list_for_each_safe(q, n, &list) {
 		tp = list_entry(q, struct tcp_sock, tsq_node);
 		list_del(&tp->tsq_node);
+		clear_bit(TSQ_QUEUED, &tp->tsq_flags);
 
 		sk = (struct sock *)tp;
-		bh_lock_sock(sk);
-
-		if (!sock_owned_by_user(sk)) {
-			tcp_tsq_handler(sk);
-		} else {
-			/* defer the work to tcp_release_cb() */
-			set_bit(TCP_TSQ_DEFERRED, &tp->tsq_flags);
+		if (!sk->sk_lock.owned &&
+		    test_bit(TCP_TSQ_DEFERRED, &tp->tsq_flags)) {
+			bh_lock_sock(sk);
+			if (!sock_owned_by_user(sk)) {
+				clear_bit(TCP_TSQ_DEFERRED, &tp->tsq_flags);
+				tcp_tsq_handler(sk);
+			}
+			bh_unlock_sock(sk);
 		}
-		bh_unlock_sock(sk);
 
-		clear_bit(TSQ_QUEUED, &tp->tsq_flags);
 		sk_free(sk);
 	}
 }
@@ -884,7 +884,7 @@ void tcp_wfree(struct sk_buff *skb)
 		if (!(oval & TSQF_THROTTLED) || (oval & TSQF_QUEUED))
 			goto out;
 
-		nval = (oval & ~TSQF_THROTTLED) | TSQF_QUEUED;
+		nval = (oval & ~TSQF_THROTTLED) | TSQF_QUEUED | TCPF_TSQ_DEFERRED;
 		nval = cmpxchg(&tp->tsq_flags, oval, nval);
 		if (nval != oval)
 			continue;
@@ -2183,6 +2183,8 @@ static bool tcp_write_xmit(struct sock *
 		    unlikely(tso_fragment(sk, skb, limit, mss_now, gfp)))
 			break;
 
+		if (test_bit(TCP_TSQ_DEFERRED, &tp->tsq_flags))
+			clear_bit(TCP_TSQ_DEFERRED, &tp->tsq_flags);
 		if (tcp_small_queue_check(sk, skb, 0))
 			break;
 
