From a2dd154377c9aa6ddda00d39b8c7c334e4fa16ff Mon Sep 17 00:00:00 2001
From: Damien Horsley <damien.horsley@imgtec.com>
Date: Tue, 22 Mar 2016 12:46:09 +0000
Subject: dmaengine: img-mdc: Handle early status read

It is possible that mdc_tx_status may be called before the first
node has been read from memory.

In this case, the residue value stored in the register is undefined.
Return the transfer size instead.

Signed-off-by: Damien Horsley <damien.horsley@imgtec.com>
---
 drivers/dma/img-mdc-dma.c | 40 ++++++++++++++++++++++++----------------
 1 file changed, 24 insertions(+), 16 deletions(-)

--- a/drivers/dma/img-mdc-dma.c
+++ b/drivers/dma/img-mdc-dma.c
@@ -623,25 +623,33 @@ static enum dma_status mdc_tx_status(str
 			(MDC_CMDS_PROCESSED_CMDS_DONE_MASK + 1);
 
 		/*
-		 * If the command loaded event hasn't been processed yet, then
-		 * the difference above includes an extra command.
+		 * If the first node has not yet been read from memory,
+		 * the residue register value is undefined
 		 */
-		if (!mdesc->cmd_loaded)
-			cmds--;
-		else
-			cmds += mdesc->list_cmds_done;
-
-		bytes = mdesc->list_xfer_size;
-		ldesc = mdesc->list;
-		for (i = 0; i < cmds; i++) {
-			bytes -= ldesc->xfer_size + 1;
-			ldesc = ldesc->next_desc;
-		}
-		if (ldesc) {
-			if (residue != MDC_TRANSFER_SIZE_MASK)
-				bytes -= ldesc->xfer_size - residue;
+		if (!mdesc->cmd_loaded && !cmds) {
+			bytes = mdesc->list_xfer_size;
+		} else {
+			/*
+			 * If the command loaded event hasn't been processed yet, then
+			 * the difference above includes an extra command.
+			 */
+			if (!mdesc->cmd_loaded)
+				cmds--;
 			else
+				cmds += mdesc->list_cmds_done;
+
+			bytes = mdesc->list_xfer_size;
+			ldesc = mdesc->list;
+			for (i = 0; i < cmds; i++) {
 				bytes -= ldesc->xfer_size + 1;
+				ldesc = ldesc->next_desc;
+			}
+			if (ldesc) {
+				if (residue != MDC_TRANSFER_SIZE_MASK)
+					bytes -= ldesc->xfer_size - residue;
+				else
+					bytes -= ldesc->xfer_size + 1;
+			}
 		}
 	}
 	spin_unlock_irqrestore(&mchan->vc.lock, flags);
