From e5327a1c6969316370af5cae7cfe6b8163178575 Mon Sep 17 00:00:00 2001
From: John Crispin <blogic@openwrt.org>
Date: Mon, 2 Dec 2013 16:07:23 +0100
Subject: [PATCH 500/507] MIPS: increase GIC_INTR_MAX

Signed-off-by: John Crispin <blogic@openwrt.org>
---
 arch/mips/include/asm/gic.h |    2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/mips/include/asm/gic.h
+++ b/arch/mips/include/asm/gic.h
@@ -19,7 +19,7 @@
 #define GIC_TRIG_EDGE			1
 #define GIC_TRIG_LEVEL			0
 
-#define GIC_NUM_INTRS			(24 + NR_CPUS * 2)
+#define GIC_NUM_INTRS			(56 + NR_CPUS * 2)
 
 #define MSK(n) ((1 << (n)) - 1)
 #define REG32(addr)		(*(volatile unsigned int *) (addr))
