From a049ce751e60451b47fa744342db84db44883e57 Mon Sep 17 00:00:00 2001
From: Pantelis Antoniou <panto@antoniou-consulting.com>
Date: Thu, 10 Jan 2013 20:37:45 +0200
Subject: [PATCH 219/752] ARM/dts: am33xx: Add mcasp0 and mcasp1 device tree
 entries

Add missing mcasp entries in the am33xx.dtsi include file.

Signed-off-by: Pantelis Antoniou <panto@antoniou-consulting.com>
Signed-off-by: Darren Etheridge <detheridge@ti.com>
Signed-off-by: Jyri Sarha <jsarha@ti.com>
---
 arch/arm/boot/dts/am33xx.dtsi |   19 +++++++++++++++++++
 1 file changed, 19 insertions(+)

--- a/arch/arm/boot/dts/am33xx.dtsi
+++ b/arch/arm/boot/dts/am33xx.dtsi
@@ -726,5 +726,24 @@
 			       <&edma 5>;
 			dma-names = "tx", "rx";
 		};
+
+		mcasp0: mcasp@48038000 {
+			compatible = "ti,omap2-mcasp-audio";
+			ti,hwmods = "mcasp0";
+			reg = <0x48038000 0x2000>;
+			interrupts = <80 81>;
+			interrupts-names = "tx", "rx";
+			status = "disabled";
+		};
+
+		mcasp1: mcasp@4803C000 {
+			compatible = "ti,omap2-mcasp-audio";
+			ti,hwmods = "mcasp1";
+			reg = <0x4803C000 0x2000>;
+			interrupts = <82 83>;
+			interrupts-names = "tx", "rx";
+			status = "disabled";
+		};
+
 	};
 };
