From dc3d88ade857ba3dca34f008e0b0aed3ef79cb15 Mon Sep 17 00:00:00 2001
From: Krzysztof Kozlowski <krzk@kernel.org>
Date: Tue, 30 Apr 2024 09:49:14 +0100
Subject: [PATCH] nvmem: sc27xx: fix module autoloading

Add MODULE_DEVICE_TABLE(), so the module could be properly autoloaded
based on the alias from of_device_id table.

Signed-off-by: Krzysztof Kozlowski <krzk@kernel.org>
Signed-off-by: Srinivas Kandagatla <srinivas.kandagatla@linaro.org>
Link: https://lore.kernel.org/r/20240430084921.33387-5-srinivas.kandagatla@linaro.org
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/nvmem/sc27xx-efuse.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/nvmem/sc27xx-efuse.c
+++ b/drivers/nvmem/sc27xx-efuse.c
@@ -263,6 +263,7 @@ static const struct of_device_id sc27xx_
 	{ .compatible = "sprd,sc2730-efuse", .data = &sc2730_edata},
 	{ }
 };
+MODULE_DEVICE_TABLE(of, sc27xx_efuse_of_match);
 
 static struct platform_driver sc27xx_efuse_driver = {
 	.probe = sc27xx_efuse_probe,
